No.     Time        Source                Destination           Protocol Info
      1 0.000000    host                  3.0                   USB      GET DESCRIPTOR Request DEVICE

Frame 1: 64 bytes on wire (512 bits), 64 bytes captured (512 bits)
    Arrival Time: Sep 21, 2011 13:56:34.466968000 CEST
    Epoch Time: 1316606194.466968000 seconds
    [Time delta from previous captured frame: 0.000000000 seconds]
    [Time delta from previous displayed frame: 0.000000000 seconds]
    [Time since reference or first frame: 0.000000000 seconds]
    Frame Number: 1
    Frame Length: 64 bytes (512 bits)
    Capture Length: 64 bytes (512 bits)
    [Frame is marked: False]
    [Frame is ignored: False]
    [Protocols in frame: usb]
USB URB
    URB id: 0x00000000ee8f5500
    URB type: URB_SUBMIT ('S')
    URB transfer type: URB_CONTROL out (0x02)
    Endpoint: 0x80
    Device: 3
    URB bus id: 1
    Device setup request: relevant (0)
    Data: not present ('<')
    URB sec: 1316606194
    URB usec: 466968
    URB status: Operation now in progress (-EINPROGRESS) (-115)
    URB length [bytes]: 40
    Data length [bytes]: 0
    [Response in: 2]
    [bInterfaceClass: Unknown (0xffff)]
    URB setup
        bmRequestType: 0x80
            1... .... = Direction: Device-to-host
            .00. .... = Type: Standard (0x00)
            ...0 0000 = Recipient: Device (0x00)
        bRequest: GET DESCRIPTOR (6)
        Descriptor Index: 0x00
        bDescriptorType: DEVICE (1)
        Language Id: no language specified (0x0000)
        wLength: 40

0000  00 55 8f ee 00 00 00 00 53 02 80 03 01 00 00 3c   .U......S......<
0010  f2 d0 79 4e 00 00 00 00 18 20 07 00 8d ff ff ff   ..yN..... ......
0020  28 00 00 00 00 00 00 00 80 06 00 01 00 00 28 00   (.............(.
0030  00 00 00 00 00 00 00 00 00 02 00 00 00 00 00 00   ................

No.     Time        Source                Destination           Protocol Info
      2 0.000263    3.0                   host                  USB      GET DESCRIPTOR Response DEVICE

Frame 2: 82 bytes on wire (656 bits), 82 bytes captured (656 bits)
    Arrival Time: Sep 21, 2011 13:56:34.467231000 CEST
    Epoch Time: 1316606194.467231000 seconds
    [Time delta from previous captured frame: 0.000263000 seconds]
    [Time delta from previous displayed frame: 0.000263000 seconds]
    [Time since reference or first frame: 0.000263000 seconds]
    Frame Number: 2
    Frame Length: 82 bytes (656 bits)
    Capture Length: 82 bytes (656 bits)
    [Frame is marked: False]
    [Frame is ignored: False]
    [Protocols in frame: usb]
USB URB
    URB id: 0x00000000ee8f5500
    URB type: URB_COMPLETE ('C')
    URB transfer type: URB_CONTROL out (0x02)
    Endpoint: 0x80
    Device: 3
    URB bus id: 1
    Device setup request: not relevant ('-')
    Data: present (0)
    URB sec: 1316606194
    URB usec: 467231
    URB status: Success (0)
    URB length [bytes]: 18
    Data length [bytes]: 18
    [Request in: 1]
    [Time from request: 0.000263000 seconds]
    [bInterfaceClass: Unknown (0xffff)]
    DEVICE DESCRIPTOR
        bLength: 18
        bDescriptorType: DEVICE (1)
        bcdUSB: 0x0200
        bDeviceClass: 0
        bDeviceSubClass: 0
        bDeviceProtocol: 0
        bMaxPacketSize0: 64
        idVendor: 0x132b
        idProduct: 0x20b8
        bcdDevice: 0x0100
        iManufacturer: 1
        iProduct: 2
        iSerialNumber: 0
        bNumConfigurations: 1

0000  00 55 8f ee 00 00 00 00 43 02 80 03 01 00 2d 00   .U......C.....-.
0010  f2 d0 79 4e 00 00 00 00 1f 21 07 00 00 00 00 00   ..yN.....!......
0020  12 00 00 00 12 00 00 00 00 00 00 00 00 00 00 00   ................
0030  00 00 00 00 00 00 00 00 00 02 00 00 00 00 00 00   ................
0040  12 01 00 02 00 00 00 40 2b 13 b8 20 00 01 01 02   .......@+.. ....
0050  00 01                                             ..

No.     Time        Source                Destination           Protocol Info
      3 0.001666    host                  1.0                   USB      GET DESCRIPTOR Request DEVICE

Frame 3: 64 bytes on wire (512 bits), 64 bytes captured (512 bits)
    Arrival Time: Sep 21, 2011 13:56:34.468634000 CEST
    Epoch Time: 1316606194.468634000 seconds
    [Time delta from previous captured frame: 0.001403000 seconds]
    [Time delta from previous displayed frame: 0.001403000 seconds]
    [Time since reference or first frame: 0.001666000 seconds]
    Frame Number: 3
    Frame Length: 64 bytes (512 bits)
    Capture Length: 64 bytes (512 bits)
    [Frame is marked: False]
    [Frame is ignored: False]
    [Protocols in frame: usb]
USB URB
    URB id: 0x00000000ee8f5500
    URB type: URB_SUBMIT ('S')
    URB transfer type: URB_CONTROL out (0x02)
    Endpoint: 0x80
    Device: 1
    URB bus id: 1
    Device setup request: relevant (0)
    Data: not present ('<')
    URB sec: 1316606194
    URB usec: 468634
    URB status: Operation now in progress (-EINPROGRESS) (-115)
    URB length [bytes]: 40
    Data length [bytes]: 0
    [Response in: 4]
    [bInterfaceClass: Unknown (0xffff)]
    URB setup
        bmRequestType: 0x80
            1... .... = Direction: Device-to-host
            .00. .... = Type: Standard (0x00)
            ...0 0000 = Recipient: Device (0x00)
        bRequest: GET DESCRIPTOR (6)
        Descriptor Index: 0x00
        bDescriptorType: DEVICE (1)
        Language Id: no language specified (0x0000)
        wLength: 40

0000  00 55 8f ee 00 00 00 00 53 02 80 01 01 00 00 3c   .U......S......<
0010  f2 d0 79 4e 00 00 00 00 9a 26 07 00 8d ff ff ff   ..yN.....&......
0020  28 00 00 00 00 00 00 00 80 06 00 01 00 00 28 00   (.............(.
0030  00 00 00 00 00 00 00 00 00 02 00 00 00 00 00 00   ................

No.     Time        Source                Destination           Protocol Info
      4 0.001672    1.0                   host                  USB      GET DESCRIPTOR Response DEVICE

Frame 4: 82 bytes on wire (656 bits), 82 bytes captured (656 bits)
    Arrival Time: Sep 21, 2011 13:56:34.468640000 CEST
    Epoch Time: 1316606194.468640000 seconds
    [Time delta from previous captured frame: 0.000006000 seconds]
    [Time delta from previous displayed frame: 0.000006000 seconds]
    [Time since reference or first frame: 0.001672000 seconds]
    Frame Number: 4
    Frame Length: 82 bytes (656 bits)
    Capture Length: 82 bytes (656 bits)
    [Frame is marked: False]
    [Frame is ignored: False]
    [Protocols in frame: usb]
USB URB
    URB id: 0x00000000ee8f5500
    URB type: URB_COMPLETE ('C')
    URB transfer type: URB_CONTROL out (0x02)
    Endpoint: 0x80
    Device: 1
    URB bus id: 1
    Device setup request: not relevant ('-')
    Data: present (0)
    URB sec: 1316606194
    URB usec: 468640
    URB status: Success (0)
    URB length [bytes]: 18
    Data length [bytes]: 18
    [Request in: 3]
    [Time from request: 0.000006000 seconds]
    [bInterfaceClass: Unknown (0xffff)]
    DEVICE DESCRIPTOR
        bLength: 18
        bDescriptorType: DEVICE (1)
        bcdUSB: 0x0200
        bDeviceClass: 9
        bDeviceSubClass: 0
        bDeviceProtocol: 0
        bMaxPacketSize0: 64
        idVendor: 0x1d6b
        idProduct: 0x0002
        bcdDevice: 0x0206
        iManufacturer: 3
        iProduct: 2
        iSerialNumber: 1
        bNumConfigurations: 1

0000  00 55 8f ee 00 00 00 00 43 02 80 01 01 00 2d 00   .U......C.....-.
0010  f2 d0 79 4e 00 00 00 00 a0 26 07 00 00 00 00 00   ..yN.....&......
0020  12 00 00 00 12 00 00 00 00 00 00 00 00 00 00 00   ................
0030  00 00 00 00 00 00 00 00 00 02 00 00 00 00 00 00   ................
0040  12 01 00 02 09 00 00 40 6b 1d 02 00 06 02 03 02   .......@k.......
0050  01 01                                             ..

No.     Time        Source                Destination           Protocol Info
      5 277.849048  1.1                   host                  USB      URB_INTERRUPT out

Frame 5: 66 bytes on wire (528 bits), 66 bytes captured (528 bits)
    Arrival Time: Sep 21, 2011 14:01:12.316016000 CEST
    Epoch Time: 1316606472.316016000 seconds
    [Time delta from previous captured frame: 277.847376000 seconds]
    [Time delta from previous displayed frame: 277.847376000 seconds]
    [Time since reference or first frame: 277.849048000 seconds]
    Frame Number: 5
    Frame Length: 66 bytes (528 bits)
    Capture Length: 66 bytes (528 bits)
    [Frame is marked: False]
    [Frame is ignored: False]
    [Protocols in frame: usb]
USB URB
    URB id: 0x00000000f3cecb80
    URB type: URB_COMPLETE ('C')
    URB transfer type: URB_INTERRUPT out (0x01)
    Endpoint: 0x81
    Device: 1
    URB bus id: 1
    Device setup request: not relevant ('-')
    Data: present (0)
    URB sec: 1316606472
    URB usec: 316016
    URB status: Success (0)
    URB length [bytes]: 2
    Data length [bytes]: 2
    Leftover Capture Data: 8000

0000  80 cb ce f3 00 00 00 00 43 01 81 01 01 00 2d 00   ........C.....-.
0010  08 d2 79 4e 00 00 00 00 70 d2 04 00 00 00 00 00   ..yN....p.......
0020  02 00 00 00 02 00 00 00 00 00 00 00 00 00 00 00   ................
0030  00 08 00 00 00 00 00 00 00 02 00 00 00 00 00 00   ................
0040  80 00                                             ..

No.     Time        Source                Destination           Protocol Info
      6 277.849061  host                  1.1                   USB      URB_INTERRUPT out

Frame 6: 64 bytes on wire (512 bits), 64 bytes captured (512 bits)
    Arrival Time: Sep 21, 2011 14:01:12.316029000 CEST
    Epoch Time: 1316606472.316029000 seconds
    [Time delta from previous captured frame: 0.000013000 seconds]
    [Time delta from previous displayed frame: 0.000013000 seconds]
    [Time since reference or first frame: 277.849061000 seconds]
    Frame Number: 6
    Frame Length: 64 bytes (512 bits)
    Capture Length: 64 bytes (512 bits)
    [Frame is marked: False]
    [Frame is ignored: False]
    [Protocols in frame: usb]
USB URB
    URB id: 0x00000000f3cecb80
    URB type: URB_SUBMIT ('S')
    URB transfer type: URB_INTERRUPT out (0x01)
    Endpoint: 0x81
    Device: 1
    URB bus id: 1
    Device setup request: not relevant ('-')
    Data: not present ('<')
    URB sec: 1316606472
    URB usec: 316029
    URB status: Operation now in progress (-EINPROGRESS) (-115)
    URB length [bytes]: 4
    Data length [bytes]: 0
    [Response in: 23]

0000  80 cb ce f3 00 00 00 00 53 01 81 01 01 00 2d 3c   ........S.....-<
0010  08 d2 79 4e 00 00 00 00 7d d2 04 00 8d ff ff ff   ..yN....}.......
0020  04 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00   ................
0030  00 08 00 00 00 00 00 00 00 02 00 00 00 00 00 00   ................

No.     Time        Source                Destination           Protocol Info
      7 277.849178  host                  1.0                   USBHUB   GET_STATUS Request

Frame 7: 64 bytes on wire (512 bits), 64 bytes captured (512 bits)
    Arrival Time: Sep 21, 2011 14:01:12.316146000 CEST
    Epoch Time: 1316606472.316146000 seconds
    [Time delta from previous captured frame: 0.000117000 seconds]
    [Time delta from previous displayed frame: 0.000117000 seconds]
    [Time since reference or first frame: 277.849178000 seconds]
    Frame Number: 7
    Frame Length: 64 bytes (512 bits)
    Capture Length: 64 bytes (512 bits)
    [Frame is marked: False]
    [Frame is ignored: False]
    [Protocols in frame: usb:usbhub]
USB URB
    URB id: 0x00000000f37ab980
    URB type: URB_SUBMIT ('S')
    URB transfer type: URB_CONTROL out (0x02)
    Endpoint: 0x80
    Device: 1
    URB bus id: 1
    Device setup request: relevant (0)
    Data: not present ('<')
    URB sec: 1316606472
    URB usec: 316146
    URB status: Operation now in progress (-EINPROGRESS) (-115)
    URB length [bytes]: 4
    Data length [bytes]: 0
    [Response in: 8]
    [bInterfaceClass: Unknown (0xffff)]
    URB setup
        bmRequestType: 0xa3
            1... .... = Direction: Device-to-host
            .01. .... = Type: Class (0x01)
            ...0 0011 = Recipient: Unknown (0x03)
    bRequest: GET_STATUS (0x00)
    wValue: 0x0000
        (zero): 0
    wIndex: 7
        Port: 7
    wLength: 4

0000  80 b9 7a f3 00 00 00 00 53 02 80 01 01 00 00 3c   ..z.....S......<
0010  08 d2 79 4e 00 00 00 00 f2 d2 04 00 8d ff ff ff   ..yN............
0020  04 00 00 00 00 00 00 00 a3 00 00 00 07 00 04 00   ................
0030  00 00 00 00 00 00 00 00 00 02 00 00 00 00 00 00   ................

No.     Time        Source                Destination           Protocol Info
      8 277.849182  1.0                   host                  USBHUB   GET_STATUS Response

Frame 8: 68 bytes on wire (544 bits), 68 bytes captured (544 bits)
    Arrival Time: Sep 21, 2011 14:01:12.316150000 CEST
    Epoch Time: 1316606472.316150000 seconds
    [Time delta from previous captured frame: 0.000004000 seconds]
    [Time delta from previous displayed frame: 0.000004000 seconds]
    [Time since reference or first frame: 277.849182000 seconds]
    Frame Number: 8
    Frame Length: 68 bytes (544 bits)
    Capture Length: 68 bytes (544 bits)
    [Frame is marked: False]
    [Frame is ignored: False]
    [Protocols in frame: usb:usbhub]
USB URB
    URB id: 0x00000000f37ab980
    URB type: URB_COMPLETE ('C')
    URB transfer type: URB_CONTROL out (0x02)
    Endpoint: 0x80
    Device: 1
    URB bus id: 1
    Device setup request: not relevant ('-')
    Data: present (0)
    URB sec: 1316606472
    URB usec: 316150
    URB status: Success (0)
    URB length [bytes]: 4
    Data length [bytes]: 4
    [Request in: 7]
    [Time from request: 0.000004000 seconds]
    [bInterfaceClass: Unknown (0xffff)]

0000  80 b9 7a f3 00 00 00 00 43 02 80 01 01 00 2d 00   ..z.....C.....-.
0010  08 d2 79 4e 00 00 00 00 f6 d2 04 00 00 00 00 00   ..yN............
0020  04 00 00 00 04 00 00 00 00 00 00 00 00 00 00 00   ................
0030  00 00 00 00 00 00 00 00 00 02 00 00 00 00 00 00   ................
0040  00 01 01 00                                       ....

No.     Time        Source                Destination           Protocol Info
      9 277.849186  host                  1.0                   USBHUB   CLEAR_FEATURE Request

Frame 9: 64 bytes on wire (512 bits), 64 bytes captured (512 bits)
    Arrival Time: Sep 21, 2011 14:01:12.316154000 CEST
    Epoch Time: 1316606472.316154000 seconds
    [Time delta from previous captured frame: 0.000004000 seconds]
    [Time delta from previous displayed frame: 0.000004000 seconds]
    [Time since reference or first frame: 277.849186000 seconds]
    Frame Number: 9
    Frame Length: 64 bytes (512 bits)
    Capture Length: 64 bytes (512 bits)
    [Frame is marked: False]
    [Frame is ignored: False]
    [Protocols in frame: usb:usbhub]
USB URB
    URB id: 0x00000000f37ab980
    URB type: URB_SUBMIT ('S')
    URB transfer type: URB_CONTROL out (0x02)
    Endpoint: 0x00
    Device: 1
    URB bus id: 1
    Device setup request: relevant (0)
    Data: present (0)
    URB sec: 1316606472
    URB usec: 316154
    URB status: Operation now in progress (-EINPROGRESS) (-115)
    URB length [bytes]: 0
    Data length [bytes]: 0
    [Response in: 10]
    [bInterfaceClass: Unknown (0xffff)]
    URB setup
        bmRequestType: 0x23
            0... .... = Direction: Host-to-device
            .01. .... = Type: Class (0x01)
            ...0 0011 = Recipient: Unknown (0x03)
    bRequest: CLEAR_FEATURE (0x01)
    wValue: 0x0010
        PortFeatureSelector: C_PORT_CONNECTION (16)
    wIndex: 7
        Port: 7
        PortSelector: 0
    wLength: 0
        (zero): 0

0000  80 b9 7a f3 00 00 00 00 53 02 00 01 01 00 00 00   ..z.....S.......
0010  08 d2 79 4e 00 00 00 00 fa d2 04 00 8d ff ff ff   ..yN............
0020  00 00 00 00 00 00 00 00 23 01 10 00 07 00 00 00   ........#.......
0030  00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00   ................

No.     Time        Source                Destination           Protocol Info
     10 277.849191  1.0                   host                  USBHUB   CLEAR_FEATURE Response

Frame 10: 64 bytes on wire (512 bits), 64 bytes captured (512 bits)
    Arrival Time: Sep 21, 2011 14:01:12.316159000 CEST
    Epoch Time: 1316606472.316159000 seconds
    [Time delta from previous captured frame: 0.000005000 seconds]
    [Time delta from previous displayed frame: 0.000005000 seconds]
    [Time since reference or first frame: 277.849191000 seconds]
    Frame Number: 10
    Frame Length: 64 bytes (512 bits)
    Capture Length: 64 bytes (512 bits)
    [Frame is marked: False]
    [Frame is ignored: False]
    [Protocols in frame: usb:usbhub]
USB URB
    URB id: 0x00000000f37ab980
    URB type: URB_COMPLETE ('C')
    URB transfer type: URB_CONTROL out (0x02)
    Endpoint: 0x00
    Device: 1
    URB bus id: 1
    Device setup request: not relevant ('-')
    Data: not present ('>')
    URB sec: 1316606472
    URB usec: 316159
    URB status: Success (0)
    URB length [bytes]: 0
    Data length [bytes]: 0
    [Request in: 9]
    [Time from request: 0.000005000 seconds]
    [bInterfaceClass: Unknown (0xffff)]

0000  80 b9 7a f3 00 00 00 00 43 02 00 01 01 00 2d 3e   ..z.....C.....->
0010  08 d2 79 4e 00 00 00 00 ff d2 04 00 00 00 00 00   ..yN............
0020  00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00   ................
0030  00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00   ................

No.     Time        Source                Destination           Protocol Info
     11 277.849494  host                  1.0                   USBHUB   GET_STATUS Request

Frame 11: 64 bytes on wire (512 bits), 64 bytes captured (512 bits)
    Arrival Time: Sep 21, 2011 14:01:12.316462000 CEST
    Epoch Time: 1316606472.316462000 seconds
    [Time delta from previous captured frame: 0.000303000 seconds]
    [Time delta from previous displayed frame: 0.000303000 seconds]
    [Time since reference or first frame: 277.849494000 seconds]
    Frame Number: 11
    Frame Length: 64 bytes (512 bits)
    Capture Length: 64 bytes (512 bits)
    [Frame is marked: False]
    [Frame is ignored: False]
    [Protocols in frame: usb:usbhub]
USB URB
    URB id: 0x00000000f37ab980
    URB type: URB_SUBMIT ('S')
    URB transfer type: URB_CONTROL out (0x02)
    Endpoint: 0x80
    Device: 1
    URB bus id: 1
    Device setup request: relevant (0)
    Data: not present ('<')
    URB sec: 1316606472
    URB usec: 316462
    URB status: Operation now in progress (-EINPROGRESS) (-115)
    URB length [bytes]: 4
    Data length [bytes]: 0
    [Response in: 12]
    [bInterfaceClass: Unknown (0xffff)]
    URB setup
        bmRequestType: 0xa3
            1... .... = Direction: Device-to-host
            .01. .... = Type: Class (0x01)
            ...0 0011 = Recipient: Unknown (0x03)
    bRequest: GET_STATUS (0x00)
    wValue: 0x0000
        (zero): 0
    wIndex: 7
        Port: 7
    wLength: 4

0000  80 b9 7a f3 00 00 00 00 53 02 80 01 01 00 00 3c   ..z.....S......<
0010  08 d2 79 4e 00 00 00 00 2e d4 04 00 8d ff ff ff   ..yN............
0020  04 00 00 00 00 00 00 00 a3 00 00 00 07 00 04 00   ................
0030  00 00 00 00 00 00 00 00 00 02 00 00 00 00 00 00   ................

No.     Time        Source                Destination           Protocol Info
     12 277.849498  1.0                   host                  USBHUB   GET_STATUS Response

Frame 12: 68 bytes on wire (544 bits), 68 bytes captured (544 bits)
    Arrival Time: Sep 21, 2011 14:01:12.316466000 CEST
    Epoch Time: 1316606472.316466000 seconds
    [Time delta from previous captured frame: 0.000004000 seconds]
    [Time delta from previous displayed frame: 0.000004000 seconds]
    [Time since reference or first frame: 277.849498000 seconds]
    Frame Number: 12
    Frame Length: 68 bytes (544 bits)
    Capture Length: 68 bytes (544 bits)
    [Frame is marked: False]
    [Frame is ignored: False]
    [Protocols in frame: usb:usbhub]
USB URB
    URB id: 0x00000000f37ab980
    URB type: URB_COMPLETE ('C')
    URB transfer type: URB_CONTROL out (0x02)
    Endpoint: 0x80
    Device: 1
    URB bus id: 1
    Device setup request: not relevant ('-')
    Data: present (0)
    URB sec: 1316606472
    URB usec: 316466
    URB status: Success (0)
    URB length [bytes]: 4
    Data length [bytes]: 4
    [Request in: 11]
    [Time from request: 0.000004000 seconds]
    [bInterfaceClass: Unknown (0xffff)]

0000  80 b9 7a f3 00 00 00 00 43 02 80 01 01 00 2d 00   ..z.....C.....-.
0010  08 d2 79 4e 00 00 00 00 32 d4 04 00 00 00 00 00   ..yN....2.......
0020  04 00 00 00 04 00 00 00 00 00 00 00 00 00 00 00   ................
0030  00 00 00 00 00 00 00 00 00 02 00 00 00 00 00 00   ................
0040  00 01 00 00                                       ....

No.     Time        Source                Destination           Protocol Info
     13 277.877598  host                  1.0                   USBHUB   GET_STATUS Request

Frame 13: 64 bytes on wire (512 bits), 64 bytes captured (512 bits)
    Arrival Time: Sep 21, 2011 14:01:12.344566000 CEST
    Epoch Time: 1316606472.344566000 seconds
    [Time delta from previous captured frame: 0.028100000 seconds]
    [Time delta from previous displayed frame: 0.028100000 seconds]
    [Time since reference or first frame: 277.877598000 seconds]
    Frame Number: 13
    Frame Length: 64 bytes (512 bits)
    Capture Length: 64 bytes (512 bits)
    [Frame is marked: False]
    [Frame is ignored: False]
    [Protocols in frame: usb:usbhub]
USB URB
    URB id: 0x00000000f37ab200
    URB type: URB_SUBMIT ('S')
    URB transfer type: URB_CONTROL out (0x02)
    Endpoint: 0x80
    Device: 1
    URB bus id: 1
    Device setup request: relevant (0)
    Data: not present ('<')
    URB sec: 1316606472
    URB usec: 344566
    URB status: Operation now in progress (-EINPROGRESS) (-115)
    URB length [bytes]: 4
    Data length [bytes]: 0
    [Response in: 14]
    [bInterfaceClass: Unknown (0xffff)]
    URB setup
        bmRequestType: 0xa3
            1... .... = Direction: Device-to-host
            .01. .... = Type: Class (0x01)
            ...0 0011 = Recipient: Unknown (0x03)
    bRequest: GET_STATUS (0x00)
    wValue: 0x0000
        (zero): 0
    wIndex: 7
        Port: 7
    wLength: 4

0000  00 b2 7a f3 00 00 00 00 53 02 80 01 01 00 00 3c   ..z.....S......<
0010  08 d2 79 4e 00 00 00 00 f6 41 05 00 8d ff ff ff   ..yN.....A......
0020  04 00 00 00 00 00 00 00 a3 00 00 00 07 00 04 00   ................
0030  00 00 00 00 00 00 00 00 00 02 00 00 00 00 00 00   ................

No.     Time        Source                Destination           Protocol Info
     14 277.877605  1.0                   host                  USBHUB   GET_STATUS Response

Frame 14: 68 bytes on wire (544 bits), 68 bytes captured (544 bits)
    Arrival Time: Sep 21, 2011 14:01:12.344573000 CEST
    Epoch Time: 1316606472.344573000 seconds
    [Time delta from previous captured frame: 0.000007000 seconds]
    [Time delta from previous displayed frame: 0.000007000 seconds]
    [Time since reference or first frame: 277.877605000 seconds]
    Frame Number: 14
    Frame Length: 68 bytes (544 bits)
    Capture Length: 68 bytes (544 bits)
    [Frame is marked: False]
    [Frame is ignored: False]
    [Protocols in frame: usb:usbhub]
USB URB
    URB id: 0x00000000f37ab200
    URB type: URB_COMPLETE ('C')
    URB transfer type: URB_CONTROL out (0x02)
    Endpoint: 0x80
    Device: 1
    URB bus id: 1
    Device setup request: not relevant ('-')
    Data: present (0)
    URB sec: 1316606472
    URB usec: 344573
    URB status: Success (0)
    URB length [bytes]: 4
    Data length [bytes]: 4
    [Request in: 13]
    [Time from request: 0.000007000 seconds]
    [bInterfaceClass: Unknown (0xffff)]

0000  00 b2 7a f3 00 00 00 00 43 02 80 01 01 00 2d 00   ..z.....C.....-.
0010  08 d2 79 4e 00 00 00 00 fd 41 05 00 00 00 00 00   ..yN.....A......
0020  04 00 00 00 04 00 00 00 00 00 00 00 00 00 00 00   ................
0030  00 00 00 00 00 00 00 00 00 02 00 00 00 00 00 00   ................
0040  00 01 00 00                                       ....

No.     Time        Source                Destination           Protocol Info
     15 277.909590  host                  1.0                   USBHUB   GET_STATUS Request

Frame 15: 64 bytes on wire (512 bits), 64 bytes captured (512 bits)
    Arrival Time: Sep 21, 2011 14:01:12.376558000 CEST
    Epoch Time: 1316606472.376558000 seconds
    [Time delta from previous captured frame: 0.031985000 seconds]
    [Time delta from previous displayed frame: 0.031985000 seconds]
    [Time since reference or first frame: 277.909590000 seconds]
    Frame Number: 15
    Frame Length: 64 bytes (512 bits)
    Capture Length: 64 bytes (512 bits)
    [Frame is marked: False]
    [Frame is ignored: False]
    [Protocols in frame: usb:usbhub]
USB URB
    URB id: 0x00000000f37ab000
    URB type: URB_SUBMIT ('S')
    URB transfer type: URB_CONTROL out (0x02)
    Endpoint: 0x80
    Device: 1
    URB bus id: 1
    Device setup request: relevant (0)
    Data: not present ('<')
    URB sec: 1316606472
    URB usec: 376558
    URB status: Operation now in progress (-EINPROGRESS) (-115)
    URB length [bytes]: 4
    Data length [bytes]: 0
    [Response in: 16]
    [bInterfaceClass: Unknown (0xffff)]
    URB setup
        bmRequestType: 0xa3
            1... .... = Direction: Device-to-host
            .01. .... = Type: Class (0x01)
            ...0 0011 = Recipient: Unknown (0x03)
    bRequest: GET_STATUS (0x00)
    wValue: 0x0000
        (zero): 0
    wIndex: 7
        Port: 7
    wLength: 4

0000  00 b0 7a f3 00 00 00 00 53 02 80 01 01 00 00 3c   ..z.....S......<
0010  08 d2 79 4e 00 00 00 00 ee be 05 00 8d ff ff ff   ..yN............
0020  04 00 00 00 00 00 00 00 a3 00 00 00 07 00 04 00   ................
0030  00 00 00 00 00 00 00 00 00 02 00 00 00 00 00 00   ................

No.     Time        Source                Destination           Protocol Info
     16 277.909598  1.0                   host                  USBHUB   GET_STATUS Response

Frame 16: 68 bytes on wire (544 bits), 68 bytes captured (544 bits)
    Arrival Time: Sep 21, 2011 14:01:12.376566000 CEST
    Epoch Time: 1316606472.376566000 seconds
    [Time delta from previous captured frame: 0.000008000 seconds]
    [Time delta from previous displayed frame: 0.000008000 seconds]
    [Time since reference or first frame: 277.909598000 seconds]
    Frame Number: 16
    Frame Length: 68 bytes (544 bits)
    Capture Length: 68 bytes (544 bits)
    [Frame is marked: False]
    [Frame is ignored: False]
    [Protocols in frame: usb:usbhub]
USB URB
    URB id: 0x00000000f37ab000
    URB type: URB_COMPLETE ('C')
    URB transfer type: URB_CONTROL out (0x02)
    Endpoint: 0x80
    Device: 1
    URB bus id: 1
    Device setup request: not relevant ('-')
    Data: present (0)
    URB sec: 1316606472
    URB usec: 376566
    URB status: Success (0)
    URB length [bytes]: 4
    Data length [bytes]: 4
    [Request in: 15]
    [Time from request: 0.000008000 seconds]
    [bInterfaceClass: Unknown (0xffff)]

0000  00 b0 7a f3 00 00 00 00 43 02 80 01 01 00 2d 00   ..z.....C.....-.
0010  08 d2 79 4e 00 00 00 00 f6 be 05 00 00 00 00 00   ..yN............
0020  04 00 00 00 04 00 00 00 00 00 00 00 00 00 00 00   ................
0030  00 00 00 00 00 00 00 00 00 02 00 00 00 00 00 00   ................
0040  00 01 00 00                                       ....

No.     Time        Source                Destination           Protocol Info
     17 277.941587  host                  1.0                   USBHUB   GET_STATUS Request

Frame 17: 64 bytes on wire (512 bits), 64 bytes captured (512 bits)
    Arrival Time: Sep 21, 2011 14:01:12.408555000 CEST
    Epoch Time: 1316606472.408555000 seconds
    [Time delta from previous captured frame: 0.031989000 seconds]
    [Time delta from previous displayed frame: 0.031989000 seconds]
    [Time since reference or first frame: 277.941587000 seconds]
    Frame Number: 17
    Frame Length: 64 bytes (512 bits)
    Capture Length: 64 bytes (512 bits)
    [Frame is marked: False]
    [Frame is ignored: False]
    [Protocols in frame: usb:usbhub]
USB URB
    URB id: 0x00000000f37ab680
    URB type: URB_SUBMIT ('S')
    URB transfer type: URB_CONTROL out (0x02)
    Endpoint: 0x80
    Device: 1
    URB bus id: 1
    Device setup request: relevant (0)
    Data: not present ('<')
    URB sec: 1316606472
    URB usec: 408555
    URB status: Operation now in progress (-EINPROGRESS) (-115)
    URB length [bytes]: 4
    Data length [bytes]: 0
    [Response in: 18]
    [bInterfaceClass: Unknown (0xffff)]
    URB setup
        bmRequestType: 0xa3
            1... .... = Direction: Device-to-host
            .01. .... = Type: Class (0x01)
            ...0 0011 = Recipient: Unknown (0x03)
    bRequest: GET_STATUS (0x00)
    wValue: 0x0000
        (zero): 0
    wIndex: 7
        Port: 7
    wLength: 4

0000  80 b6 7a f3 00 00 00 00 53 02 80 01 01 00 00 3c   ..z.....S......<
0010  08 d2 79 4e 00 00 00 00 eb 3b 06 00 8d ff ff ff   ..yN.....;......
0020  04 00 00 00 00 00 00 00 a3 00 00 00 07 00 04 00   ................
0030  00 00 00 00 00 00 00 00 00 02 00 00 00 00 00 00   ................

No.     Time        Source                Destination           Protocol Info
     18 277.941597  1.0                   host                  USBHUB   GET_STATUS Response

Frame 18: 68 bytes on wire (544 bits), 68 bytes captured (544 bits)
    Arrival Time: Sep 21, 2011 14:01:12.408565000 CEST
    Epoch Time: 1316606472.408565000 seconds
    [Time delta from previous captured frame: 0.000010000 seconds]
    [Time delta from previous displayed frame: 0.000010000 seconds]
    [Time since reference or first frame: 277.941597000 seconds]
    Frame Number: 18
    Frame Length: 68 bytes (544 bits)
    Capture Length: 68 bytes (544 bits)
    [Frame is marked: False]
    [Frame is ignored: False]
    [Protocols in frame: usb:usbhub]
USB URB
    URB id: 0x00000000f37ab680
    URB type: URB_COMPLETE ('C')
    URB transfer type: URB_CONTROL out (0x02)
    Endpoint: 0x80
    Device: 1
    URB bus id: 1
    Device setup request: not relevant ('-')
    Data: present (0)
    URB sec: 1316606472
    URB usec: 408565
    URB status: Success (0)
    URB length [bytes]: 4
    Data length [bytes]: 4
    [Request in: 17]
    [Time from request: 0.000010000 seconds]
    [bInterfaceClass: Unknown (0xffff)]

0000  80 b6 7a f3 00 00 00 00 43 02 80 01 01 00 2d 00   ..z.....C.....-.
0010  08 d2 79 4e 00 00 00 00 f5 3b 06 00 00 00 00 00   ..yN.....;......
0020  04 00 00 00 04 00 00 00 00 00 00 00 00 00 00 00   ................
0030  00 00 00 00 00 00 00 00 00 02 00 00 00 00 00 00   ................
0040  00 01 00 00                                       ....

No.     Time        Source                Destination           Protocol Info
     19 277.973585  host                  1.0                   USBHUB   GET_STATUS Request

Frame 19: 64 bytes on wire (512 bits), 64 bytes captured (512 bits)
    Arrival Time: Sep 21, 2011 14:01:12.440553000 CEST
    Epoch Time: 1316606472.440553000 seconds
    [Time delta from previous captured frame: 0.031988000 seconds]
    [Time delta from previous displayed frame: 0.031988000 seconds]
    [Time since reference or first frame: 277.973585000 seconds]
    Frame Number: 19
    Frame Length: 64 bytes (512 bits)
    Capture Length: 64 bytes (512 bits)
    [Frame is marked: False]
    [Frame is ignored: False]
    [Protocols in frame: usb:usbhub]
USB URB
    URB id: 0x00000000f37ab680
    URB type: URB_SUBMIT ('S')
    URB transfer type: URB_CONTROL out (0x02)
    Endpoint: 0x80
    Device: 1
    URB bus id: 1
    Device setup request: relevant (0)
    Data: not present ('<')
    URB sec: 1316606472
    URB usec: 440553
    URB status: Operation now in progress (-EINPROGRESS) (-115)
    URB length [bytes]: 4
    Data length [bytes]: 0
    [Response in: 20]
    [bInterfaceClass: Unknown (0xffff)]
    URB setup
        bmRequestType: 0xa3
            1... .... = Direction: Device-to-host
            .01. .... = Type: Class (0x01)
            ...0 0011 = Recipient: Unknown (0x03)
    bRequest: GET_STATUS (0x00)
    wValue: 0x0000
        (zero): 0
    wIndex: 7
        Port: 7
    wLength: 4

0000  80 b6 7a f3 00 00 00 00 53 02 80 01 01 00 00 3c   ..z.....S......<
0010  08 d2 79 4e 00 00 00 00 e9 b8 06 00 8d ff ff ff   ..yN............
0020  04 00 00 00 00 00 00 00 a3 00 00 00 07 00 04 00   ................
0030  00 00 00 00 00 00 00 00 00 02 00 00 00 00 00 00   ................

No.     Time        Source                Destination           Protocol Info
     20 277.973596  1.0                   host                  USBHUB   GET_STATUS Response

Frame 20: 68 bytes on wire (544 bits), 68 bytes captured (544 bits)
    Arrival Time: Sep 21, 2011 14:01:12.440564000 CEST
    Epoch Time: 1316606472.440564000 seconds
    [Time delta from previous captured frame: 0.000011000 seconds]
    [Time delta from previous displayed frame: 0.000011000 seconds]
    [Time since reference or first frame: 277.973596000 seconds]
    Frame Number: 20
    Frame Length: 68 bytes (544 bits)
    Capture Length: 68 bytes (544 bits)
    [Frame is marked: False]
    [Frame is ignored: False]
    [Protocols in frame: usb:usbhub]
USB URB
    URB id: 0x00000000f37ab680
    URB type: URB_COMPLETE ('C')
    URB transfer type: URB_CONTROL out (0x02)
    Endpoint: 0x80
    Device: 1
    URB bus id: 1
    Device setup request: not relevant ('-')
    Data: present (0)
    URB sec: 1316606472
    URB usec: 440564
    URB status: Success (0)
    URB length [bytes]: 4
    Data length [bytes]: 4
    [Request in: 19]
    [Time from request: 0.000011000 seconds]
    [bInterfaceClass: Unknown (0xffff)]

0000  80 b6 7a f3 00 00 00 00 43 02 80 01 01 00 2d 00   ..z.....C.....-.
0010  08 d2 79 4e 00 00 00 00 f4 b8 06 00 00 00 00 00   ..yN............
0020  04 00 00 00 04 00 00 00 00 00 00 00 00 00 00 00   ................
0030  00 00 00 00 00 00 00 00 00 02 00 00 00 00 00 00   ................
0040  00 01 00 00                                       ....

No.     Time        Source                Destination           Protocol Info
     21 277.973601  host                  1.0                   USBHUB   GET_STATUS Request

Frame 21: 64 bytes on wire (512 bits), 64 bytes captured (512 bits)
    Arrival Time: Sep 21, 2011 14:01:12.440569000 CEST
    Epoch Time: 1316606472.440569000 seconds
    [Time delta from previous captured frame: 0.000005000 seconds]
    [Time delta from previous displayed frame: 0.000005000 seconds]
    [Time since reference or first frame: 277.973601000 seconds]
    Frame Number: 21
    Frame Length: 64 bytes (512 bits)
    Capture Length: 64 bytes (512 bits)
    [Frame is marked: False]
    [Frame is ignored: False]
    [Protocols in frame: usb:usbhub]
USB URB
    URB id: 0x00000000f37ab680
    URB type: URB_SUBMIT ('S')
    URB transfer type: URB_CONTROL out (0x02)
    Endpoint: 0x80
    Device: 1
    URB bus id: 1
    Device setup request: relevant (0)
    Data: not present ('<')
    URB sec: 1316606472
    URB usec: 440569
    URB status: Operation now in progress (-EINPROGRESS) (-115)
    URB length [bytes]: 4
    Data length [bytes]: 0
    [Response in: 22]
    [bInterfaceClass: Unknown (0xffff)]
    URB setup
        bmRequestType: 0xa3
            1... .... = Direction: Device-to-host
            .01. .... = Type: Class (0x01)
            ...0 0011 = Recipient: Unknown (0x03)
    bRequest: GET_STATUS (0x00)
    wValue: 0x0000
        (zero): 0
    wIndex: 8
        Port: 8
    wLength: 4

0000  80 b6 7a f3 00 00 00 00 53 02 80 01 01 00 00 3c   ..z.....S......<
0010  08 d2 79 4e 00 00 00 00 f9 b8 06 00 8d ff ff ff   ..yN............
0020  04 00 00 00 00 00 00 00 a3 00 00 00 08 00 04 00   ................
0030  00 00 00 00 00 00 00 00 00 02 00 00 00 00 00 00   ................

No.     Time        Source                Destination           Protocol Info
     22 277.973605  1.0                   host                  USBHUB   GET_STATUS Response

Frame 22: 68 bytes on wire (544 bits), 68 bytes captured (544 bits)
    Arrival Time: Sep 21, 2011 14:01:12.440573000 CEST
    Epoch Time: 1316606472.440573000 seconds
    [Time delta from previous captured frame: 0.000004000 seconds]
    [Time delta from previous displayed frame: 0.000004000 seconds]
    [Time since reference or first frame: 277.973605000 seconds]
    Frame Number: 22
    Frame Length: 68 bytes (544 bits)
    Capture Length: 68 bytes (544 bits)
    [Frame is marked: False]
    [Frame is ignored: False]
    [Protocols in frame: usb:usbhub]
USB URB
    URB id: 0x00000000f37ab680
    URB type: URB_COMPLETE ('C')
    URB transfer type: URB_CONTROL out (0x02)
    Endpoint: 0x80
    Device: 1
    URB bus id: 1
    Device setup request: not relevant ('-')
    Data: present (0)
    URB sec: 1316606472
    URB usec: 440573
    URB status: Success (0)
    URB length [bytes]: 4
    Data length [bytes]: 4
    [Request in: 21]
    [Time from request: 0.000004000 seconds]
    [bInterfaceClass: Unknown (0xffff)]

0000  80 b6 7a f3 00 00 00 00 43 02 80 01 01 00 2d 00   ..z.....C.....-.
0010  08 d2 79 4e 00 00 00 00 fd b8 06 00 00 00 00 00   ..yN............
0020  04 00 00 00 04 00 00 00 00 00 00 00 00 00 00 00   ................
0030  00 00 00 00 00 00 00 00 00 02 00 00 00 00 00 00   ................
0040  00 01 00 00                                       ....

No.     Time        Source                Destination           Protocol Info
     23 279.973632  1.1                   host                  USB      URB_INTERRUPT out

Frame 23: 64 bytes on wire (512 bits), 64 bytes captured (512 bits)
    Arrival Time: Sep 21, 2011 14:01:14.440600000 CEST
    Epoch Time: 1316606474.440600000 seconds
    [Time delta from previous captured frame: 2.000027000 seconds]
    [Time delta from previous displayed frame: 2.000027000 seconds]
    [Time since reference or first frame: 279.973632000 seconds]
    Frame Number: 23
    Frame Length: 64 bytes (512 bits)
    Capture Length: 64 bytes (512 bits)
    [Frame is marked: False]
    [Frame is ignored: False]
    [Protocols in frame: usb]
USB URB
    URB id: 0x00000000f3cecb80
    URB type: URB_COMPLETE ('C')
    URB transfer type: URB_INTERRUPT out (0x01)
    Endpoint: 0x81
    Device: 1
    URB bus id: 1
    Device setup request: not relevant ('-')
    Data: present (0)
    URB sec: 1316606474
    URB usec: 440600
    URB status: No such file or directory (-ENOENT) (-2)
    URB length [bytes]: 0
    Data length [bytes]: 0
    [Request in: 6]
    [Time from request: 2.124571000 seconds]

0000  80 cb ce f3 00 00 00 00 43 01 81 01 01 00 2d 00   ........C.....-.
0010  0a d2 79 4e 00 00 00 00 18 b9 06 00 fe ff ff ff   ..yN............
0020  00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00   ................
0030  00 08 00 00 00 00 00 00 00 02 00 00 00 00 00 00   ................

No.     Time        Source                Destination           Protocol Info
     24 364.309615  host                  1.0                   USBHUB   GET_STATUS Request

Frame 24: 64 bytes on wire (512 bits), 64 bytes captured (512 bits)
    Arrival Time: Sep 21, 2011 14:02:38.776583000 CEST
    Epoch Time: 1316606558.776583000 seconds
    [Time delta from previous captured frame: 84.335983000 seconds]
    [Time delta from previous displayed frame: 84.335983000 seconds]
    [Time since reference or first frame: 364.309615000 seconds]
    Frame Number: 24
    Frame Length: 64 bytes (512 bits)
    Capture Length: 64 bytes (512 bits)
    [Frame is marked: False]
    [Frame is ignored: False]
    [Protocols in frame: usb:usbhub]
USB URB
    URB id: 0x00000000f37ab080
    URB type: URB_SUBMIT ('S')
    URB transfer type: URB_CONTROL out (0x02)
    Endpoint: 0x80
    Device: 1
    URB bus id: 1
    Device setup request: relevant (0)
    Data: not present ('<')
    URB sec: 1316606558
    URB usec: 776583
    URB status: Operation now in progress (-EINPROGRESS) (-115)
    URB length [bytes]: 4
    Data length [bytes]: 0
    [Response in: 25]
    [bInterfaceClass: Unknown (0xffff)]
    URB setup
        bmRequestType: 0xa3
            1... .... = Direction: Device-to-host
            .01. .... = Type: Class (0x01)
            ...0 0011 = Recipient: Unknown (0x03)
    bRequest: GET_STATUS (0x00)
    wValue: 0x0000
        (zero): 0
    wIndex: 1
        Port: 1
    wLength: 4

0000  80 b0 7a f3 00 00 00 00 53 02 80 01 01 00 00 3c   ..z.....S......<
0010  5e d2 79 4e 00 00 00 00 87 d9 0b 00 8d ff ff ff   ^.yN............
0020  04 00 00 00 00 00 00 00 a3 00 00 00 01 00 04 00   ................
0030  00 00 00 00 00 00 00 00 00 02 00 00 00 00 00 00   ................

No.     Time        Source                Destination           Protocol Info
     25 364.309631  1.0                   host                  USBHUB   GET_STATUS Response

Frame 25: 68 bytes on wire (544 bits), 68 bytes captured (544 bits)
    Arrival Time: Sep 21, 2011 14:02:38.776599000 CEST
    Epoch Time: 1316606558.776599000 seconds
    [Time delta from previous captured frame: 0.000016000 seconds]
    [Time delta from previous displayed frame: 0.000016000 seconds]
    [Time since reference or first frame: 364.309631000 seconds]
    Frame Number: 25
    Frame Length: 68 bytes (544 bits)
    Capture Length: 68 bytes (544 bits)
    [Frame is marked: False]
    [Frame is ignored: False]
    [Protocols in frame: usb:usbhub]
USB URB
    URB id: 0x00000000f37ab080
    URB type: URB_COMPLETE ('C')
    URB transfer type: URB_CONTROL out (0x02)
    Endpoint: 0x80
    Device: 1
    URB bus id: 1
    Device setup request: not relevant ('-')
    Data: present (0)
    URB sec: 1316606558
    URB usec: 776599
    URB status: Success (0)
    URB length [bytes]: 4
    Data length [bytes]: 4
    [Request in: 24]
    [Time from request: 0.000016000 seconds]
    [bInterfaceClass: Unknown (0xffff)]

0000  80 b0 7a f3 00 00 00 00 43 02 80 01 01 00 2d 00   ..z.....C.....-.
0010  5e d2 79 4e 00 00 00 00 97 d9 0b 00 00 00 00 00   ^.yN............
0020  04 00 00 00 04 00 00 00 00 00 00 00 00 00 00 00   ................
0030  00 00 00 00 00 00 00 00 00 02 00 00 00 00 00 00   ................
0040  00 01 00 00                                       ....

No.     Time        Source                Destination           Protocol Info
     26 364.309637  host                  1.0                   USBHUB   GET_STATUS Request

Frame 26: 64 bytes on wire (512 bits), 64 bytes captured (512 bits)
    Arrival Time: Sep 21, 2011 14:02:38.776605000 CEST
    Epoch Time: 1316606558.776605000 seconds
    [Time delta from previous captured frame: 0.000006000 seconds]
    [Time delta from previous displayed frame: 0.000006000 seconds]
    [Time since reference or first frame: 364.309637000 seconds]
    Frame Number: 26
    Frame Length: 64 bytes (512 bits)
    Capture Length: 64 bytes (512 bits)
    [Frame is marked: False]
    [Frame is ignored: False]
    [Protocols in frame: usb:usbhub]
USB URB
    URB id: 0x00000000f37ab080
    URB type: URB_SUBMIT ('S')
    URB transfer type: URB_CONTROL out (0x02)
    Endpoint: 0x80
    Device: 1
    URB bus id: 1
    Device setup request: relevant (0)
    Data: not present ('<')
    URB sec: 1316606558
    URB usec: 776605
    URB status: Operation now in progress (-EINPROGRESS) (-115)
    URB length [bytes]: 4
    Data length [bytes]: 0
    [Response in: 27]
    [bInterfaceClass: Unknown (0xffff)]
    URB setup
        bmRequestType: 0xa3
            1... .... = Direction: Device-to-host
            .01. .... = Type: Class (0x01)
            ...0 0011 = Recipient: Unknown (0x03)
    bRequest: GET_STATUS (0x00)
    wValue: 0x0000
        (zero): 0
    wIndex: 2
        Port: 2
    wLength: 4

0000  80 b0 7a f3 00 00 00 00 53 02 80 01 01 00 00 3c   ..z.....S......<
0010  5e d2 79 4e 00 00 00 00 9d d9 0b 00 8d ff ff ff   ^.yN............
0020  04 00 00 00 00 00 00 00 a3 00 00 00 02 00 04 00   ................
0030  00 00 00 00 00 00 00 00 00 02 00 00 00 00 00 00   ................

No.     Time        Source                Destination           Protocol Info
     27 364.309644  1.0                   host                  USBHUB   GET_STATUS Response

Frame 27: 68 bytes on wire (544 bits), 68 bytes captured (544 bits)
    Arrival Time: Sep 21, 2011 14:02:38.776612000 CEST
    Epoch Time: 1316606558.776612000 seconds
    [Time delta from previous captured frame: 0.000007000 seconds]
    [Time delta from previous displayed frame: 0.000007000 seconds]
    [Time since reference or first frame: 364.309644000 seconds]
    Frame Number: 27
    Frame Length: 68 bytes (544 bits)
    Capture Length: 68 bytes (544 bits)
    [Frame is marked: False]
    [Frame is ignored: False]
    [Protocols in frame: usb:usbhub]
USB URB
    URB id: 0x00000000f37ab080
    URB type: URB_COMPLETE ('C')
    URB transfer type: URB_CONTROL out (0x02)
    Endpoint: 0x80
    Device: 1
    URB bus id: 1
    Device setup request: not relevant ('-')
    Data: present (0)
    URB sec: 1316606558
    URB usec: 776612
    URB status: Success (0)
    URB length [bytes]: 4
    Data length [bytes]: 4
    [Request in: 26]
    [Time from request: 0.000007000 seconds]
    [bInterfaceClass: Unknown (0xffff)]

0000  80 b0 7a f3 00 00 00 00 43 02 80 01 01 00 2d 00   ..z.....C.....-.
0010  5e d2 79 4e 00 00 00 00 a4 d9 0b 00 00 00 00 00   ^.yN............
0020  04 00 00 00 04 00 00 00 00 00 00 00 00 00 00 00   ................
0030  00 00 00 00 00 00 00 00 00 02 00 00 00 00 00 00   ................
0040  00 01 00 00                                       ....

No.     Time        Source                Destination           Protocol Info
     28 364.309648  host                  1.0                   USBHUB   GET_STATUS Request

Frame 28: 64 bytes on wire (512 bits), 64 bytes captured (512 bits)
    Arrival Time: Sep 21, 2011 14:02:38.776616000 CEST
    Epoch Time: 1316606558.776616000 seconds
    [Time delta from previous captured frame: 0.000004000 seconds]
    [Time delta from previous displayed frame: 0.000004000 seconds]
    [Time since reference or first frame: 364.309648000 seconds]
    Frame Number: 28
    Frame Length: 64 bytes (512 bits)
    Capture Length: 64 bytes (512 bits)
    [Frame is marked: False]
    [Frame is ignored: False]
    [Protocols in frame: usb:usbhub]
USB URB
    URB id: 0x00000000f37ab080
    URB type: URB_SUBMIT ('S')
    URB transfer type: URB_CONTROL out (0x02)
    Endpoint: 0x80
    Device: 1
    URB bus id: 1
    Device setup request: relevant (0)
    Data: not present ('<')
    URB sec: 1316606558
    URB usec: 776616
    URB status: Operation now in progress (-EINPROGRESS) (-115)
    URB length [bytes]: 4
    Data length [bytes]: 0
    [Response in: 29]
    [bInterfaceClass: Unknown (0xffff)]
    URB setup
        bmRequestType: 0xa3
            1... .... = Direction: Device-to-host
            .01. .... = Type: Class (0x01)
            ...0 0011 = Recipient: Unknown (0x03)
    bRequest: GET_STATUS (0x00)
    wValue: 0x0000
        (zero): 0
    wIndex: 3
        Port: 3
    wLength: 4

0000  80 b0 7a f3 00 00 00 00 53 02 80 01 01 00 00 3c   ..z.....S......<
0010  5e d2 79 4e 00 00 00 00 a8 d9 0b 00 8d ff ff ff   ^.yN............
0020  04 00 00 00 00 00 00 00 a3 00 00 00 03 00 04 00   ................
0030  00 00 00 00 00 00 00 00 00 02 00 00 00 00 00 00   ................

No.     Time        Source                Destination           Protocol Info
     29 364.309652  1.0                   host                  USBHUB   GET_STATUS Response

Frame 29: 68 bytes on wire (544 bits), 68 bytes captured (544 bits)
    Arrival Time: Sep 21, 2011 14:02:38.776620000 CEST
    Epoch Time: 1316606558.776620000 seconds
    [Time delta from previous captured frame: 0.000004000 seconds]
    [Time delta from previous displayed frame: 0.000004000 seconds]
    [Time since reference or first frame: 364.309652000 seconds]
    Frame Number: 29
    Frame Length: 68 bytes (544 bits)
    Capture Length: 68 bytes (544 bits)
    [Frame is marked: False]
    [Frame is ignored: False]
    [Protocols in frame: usb:usbhub]
USB URB
    URB id: 0x00000000f37ab080
    URB type: URB_COMPLETE ('C')
    URB transfer type: URB_CONTROL out (0x02)
    Endpoint: 0x80
    Device: 1
    URB bus id: 1
    Device setup request: not relevant ('-')
    Data: present (0)
    URB sec: 1316606558
    URB usec: 776620
    URB status: Success (0)
    URB length [bytes]: 4
    Data length [bytes]: 4
    [Request in: 28]
    [Time from request: 0.000004000 seconds]
    [bInterfaceClass: Unknown (0xffff)]

0000  80 b0 7a f3 00 00 00 00 43 02 80 01 01 00 2d 00   ..z.....C.....-.
0010  5e d2 79 4e 00 00 00 00 ac d9 0b 00 00 00 00 00   ^.yN............
0020  04 00 00 00 04 00 00 00 00 00 00 00 00 00 00 00   ................
0030  00 00 00 00 00 00 00 00 00 02 00 00 00 00 00 00   ................
0040  00 01 00 00                                       ....

No.     Time        Source                Destination           Protocol Info
     30 364.309655  host                  1.0                   USBHUB   GET_STATUS Request

Frame 30: 64 bytes on wire (512 bits), 64 bytes captured (512 bits)
    Arrival Time: Sep 21, 2011 14:02:38.776623000 CEST
    Epoch Time: 1316606558.776623000 seconds
    [Time delta from previous captured frame: 0.000003000 seconds]
    [Time delta from previous displayed frame: 0.000003000 seconds]
    [Time since reference or first frame: 364.309655000 seconds]
    Frame Number: 30
    Frame Length: 64 bytes (512 bits)
    Capture Length: 64 bytes (512 bits)
    [Frame is marked: False]
    [Frame is ignored: False]
    [Protocols in frame: usb:usbhub]
USB URB
    URB id: 0x00000000f37ab080
    URB type: URB_SUBMIT ('S')
    URB transfer type: URB_CONTROL out (0x02)
    Endpoint: 0x80
    Device: 1
    URB bus id: 1
    Device setup request: relevant (0)
    Data: not present ('<')
    URB sec: 1316606558
    URB usec: 776623
    URB status: Operation now in progress (-EINPROGRESS) (-115)
    URB length [bytes]: 4
    Data length [bytes]: 0
    [Response in: 31]
    [bInterfaceClass: Unknown (0xffff)]
    URB setup
        bmRequestType: 0xa3
            1... .... = Direction: Device-to-host
            .01. .... = Type: Class (0x01)
            ...0 0011 = Recipient: Unknown (0x03)
    bRequest: GET_STATUS (0x00)
    wValue: 0x0000
        (zero): 0
    wIndex: 4
        Port: 4
    wLength: 4

0000  80 b0 7a f3 00 00 00 00 53 02 80 01 01 00 00 3c   ..z.....S......<
0010  5e d2 79 4e 00 00 00 00 af d9 0b 00 8d ff ff ff   ^.yN............
0020  04 00 00 00 00 00 00 00 a3 00 00 00 04 00 04 00   ................
0030  00 00 00 00 00 00 00 00 00 02 00 00 00 00 00 00   ................

No.     Time        Source                Destination           Protocol Info
     31 364.309660  1.0                   host                  USBHUB   GET_STATUS Response

Frame 31: 68 bytes on wire (544 bits), 68 bytes captured (544 bits)
    Arrival Time: Sep 21, 2011 14:02:38.776628000 CEST
    Epoch Time: 1316606558.776628000 seconds
    [Time delta from previous captured frame: 0.000005000 seconds]
    [Time delta from previous displayed frame: 0.000005000 seconds]
    [Time since reference or first frame: 364.309660000 seconds]
    Frame Number: 31
    Frame Length: 68 bytes (544 bits)
    Capture Length: 68 bytes (544 bits)
    [Frame is marked: False]
    [Frame is ignored: False]
    [Protocols in frame: usb:usbhub]
USB URB
    URB id: 0x00000000f37ab080
    URB type: URB_COMPLETE ('C')
    URB transfer type: URB_CONTROL out (0x02)
    Endpoint: 0x80
    Device: 1
    URB bus id: 1
    Device setup request: not relevant ('-')
    Data: present (0)
    URB sec: 1316606558
    URB usec: 776628
    URB status: Success (0)
    URB length [bytes]: 4
    Data length [bytes]: 4
    [Request in: 30]
    [Time from request: 0.000005000 seconds]
    [bInterfaceClass: Unknown (0xffff)]

0000  80 b0 7a f3 00 00 00 00 43 02 80 01 01 00 2d 00   ..z.....C.....-.
0010  5e d2 79 4e 00 00 00 00 b4 d9 0b 00 00 00 00 00   ^.yN............
0020  04 00 00 00 04 00 00 00 00 00 00 00 00 00 00 00   ................
0030  00 00 00 00 00 00 00 00 00 02 00 00 00 00 00 00   ................
0040  00 01 00 00                                       ....

No.     Time        Source                Destination           Protocol Info
     32 364.309663  host                  1.0                   USBHUB   GET_STATUS Request

Frame 32: 64 bytes on wire (512 bits), 64 bytes captured (512 bits)
    Arrival Time: Sep 21, 2011 14:02:38.776631000 CEST
    Epoch Time: 1316606558.776631000 seconds
    [Time delta from previous captured frame: 0.000003000 seconds]
    [Time delta from previous displayed frame: 0.000003000 seconds]
    [Time since reference or first frame: 364.309663000 seconds]
    Frame Number: 32
    Frame Length: 64 bytes (512 bits)
    Capture Length: 64 bytes (512 bits)
    [Frame is marked: False]
    [Frame is ignored: False]
    [Protocols in frame: usb:usbhub]
USB URB
    URB id: 0x00000000f37ab080
    URB type: URB_SUBMIT ('S')
    URB transfer type: URB_CONTROL out (0x02)
    Endpoint: 0x80
    Device: 1
    URB bus id: 1
    Device setup request: relevant (0)
    Data: not present ('<')
    URB sec: 1316606558
    URB usec: 776631
    URB status: Operation now in progress (-EINPROGRESS) (-115)
    URB length [bytes]: 4
    Data length [bytes]: 0
    [Response in: 33]
    [bInterfaceClass: Unknown (0xffff)]
    URB setup
        bmRequestType: 0xa3
            1... .... = Direction: Device-to-host
            .01. .... = Type: Class (0x01)
            ...0 0011 = Recipient: Unknown (0x03)
    bRequest: GET_STATUS (0x00)
    wValue: 0x0000
        (zero): 0
    wIndex: 5
        Port: 5
    wLength: 4

0000  80 b0 7a f3 00 00 00 00 53 02 80 01 01 00 00 3c   ..z.....S......<
0010  5e d2 79 4e 00 00 00 00 b7 d9 0b 00 8d ff ff ff   ^.yN............
0020  04 00 00 00 00 00 00 00 a3 00 00 00 05 00 04 00   ................
0030  00 00 00 00 00 00 00 00 00 02 00 00 00 00 00 00   ................

No.     Time        Source                Destination           Protocol Info
     33 364.309668  1.0                   host                  USBHUB   GET_STATUS Response

Frame 33: 68 bytes on wire (544 bits), 68 bytes captured (544 bits)
    Arrival Time: Sep 21, 2011 14:02:38.776636000 CEST
    Epoch Time: 1316606558.776636000 seconds
    [Time delta from previous captured frame: 0.000005000 seconds]
    [Time delta from previous displayed frame: 0.000005000 seconds]
    [Time since reference or first frame: 364.309668000 seconds]
    Frame Number: 33
    Frame Length: 68 bytes (544 bits)
    Capture Length: 68 bytes (544 bits)
    [Frame is marked: False]
    [Frame is ignored: False]
    [Protocols in frame: usb:usbhub]
USB URB
    URB id: 0x00000000f37ab080
    URB type: URB_COMPLETE ('C')
    URB transfer type: URB_CONTROL out (0x02)
    Endpoint: 0x80
    Device: 1
    URB bus id: 1
    Device setup request: not relevant ('-')
    Data: present (0)
    URB sec: 1316606558
    URB usec: 776636
    URB status: Success (0)
    URB length [bytes]: 4
    Data length [bytes]: 4
    [Request in: 32]
    [Time from request: 0.000005000 seconds]
    [bInterfaceClass: Unknown (0xffff)]

0000  80 b0 7a f3 00 00 00 00 43 02 80 01 01 00 2d 00   ..z.....C.....-.
0010  5e d2 79 4e 00 00 00 00 bc d9 0b 00 00 00 00 00   ^.yN............
0020  04 00 00 00 04 00 00 00 00 00 00 00 00 00 00 00   ................
0030  00 00 00 00 00 00 00 00 00 02 00 00 00 00 00 00   ................
0040  01 05 01 00                                       ....

No.     Time        Source                Destination           Protocol Info
     34 364.309671  host                  1.0                   USBHUB   CLEAR_FEATURE Request

Frame 34: 64 bytes on wire (512 bits), 64 bytes captured (512 bits)
    Arrival Time: Sep 21, 2011 14:02:38.776639000 CEST
    Epoch Time: 1316606558.776639000 seconds
    [Time delta from previous captured frame: 0.000003000 seconds]
    [Time delta from previous displayed frame: 0.000003000 seconds]
    [Time since reference or first frame: 364.309671000 seconds]
    Frame Number: 34
    Frame Length: 64 bytes (512 bits)
    Capture Length: 64 bytes (512 bits)
    [Frame is marked: False]
    [Frame is ignored: False]
    [Protocols in frame: usb:usbhub]
USB URB
    URB id: 0x00000000f37ab080
    URB type: URB_SUBMIT ('S')
    URB transfer type: URB_CONTROL out (0x02)
    Endpoint: 0x00
    Device: 1
    URB bus id: 1
    Device setup request: relevant (0)
    Data: present (0)
    URB sec: 1316606558
    URB usec: 776639
    URB status: Operation now in progress (-EINPROGRESS) (-115)
    URB length [bytes]: 0
    Data length [bytes]: 0
    [Response in: 35]
    [bInterfaceClass: Unknown (0xffff)]
    URB setup
        bmRequestType: 0x23
            0... .... = Direction: Host-to-device
            .01. .... = Type: Class (0x01)
            ...0 0011 = Recipient: Unknown (0x03)
    bRequest: CLEAR_FEATURE (0x01)
    wValue: 0x0010
        PortFeatureSelector: C_PORT_CONNECTION (16)
    wIndex: 5
        Port: 5
        PortSelector: 0
    wLength: 0
        (zero): 0

0000  80 b0 7a f3 00 00 00 00 53 02 00 01 01 00 00 00   ..z.....S.......
0010  5e d2 79 4e 00 00 00 00 bf d9 0b 00 8d ff ff ff   ^.yN............
0020  00 00 00 00 00 00 00 00 23 01 10 00 05 00 00 00   ........#.......
0030  00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00   ................

No.     Time        Source                Destination           Protocol Info
     35 364.309677  1.0                   host                  USBHUB   CLEAR_FEATURE Response

Frame 35: 64 bytes on wire (512 bits), 64 bytes captured (512 bits)
    Arrival Time: Sep 21, 2011 14:02:38.776645000 CEST
    Epoch Time: 1316606558.776645000 seconds
    [Time delta from previous captured frame: 0.000006000 seconds]
    [Time delta from previous displayed frame: 0.000006000 seconds]
    [Time since reference or first frame: 364.309677000 seconds]
    Frame Number: 35
    Frame Length: 64 bytes (512 bits)
    Capture Length: 64 bytes (512 bits)
    [Frame is marked: False]
    [Frame is ignored: False]
    [Protocols in frame: usb:usbhub]
USB URB
    URB id: 0x00000000f37ab080
    URB type: URB_COMPLETE ('C')
    URB transfer type: URB_CONTROL out (0x02)
    Endpoint: 0x00
    Device: 1
    URB bus id: 1
    Device setup request: not relevant ('-')
    Data: not present ('>')
    URB sec: 1316606558
    URB usec: 776645
    URB status: Success (0)
    URB length [bytes]: 0
    Data length [bytes]: 0
    [Request in: 34]
    [Time from request: 0.000006000 seconds]
    [bInterfaceClass: Unknown (0xffff)]

0000  80 b0 7a f3 00 00 00 00 43 02 00 01 01 00 2d 3e   ..z.....C.....->
0010  5e d2 79 4e 00 00 00 00 c5 d9 0b 00 00 00 00 00   ^.yN............
0020  00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00   ................
0030  00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00   ................

No.     Time        Source                Destination           Protocol Info
     36 364.309680  host                  1.0                   USBHUB   GET_STATUS Request

Frame 36: 64 bytes on wire (512 bits), 64 bytes captured (512 bits)
    Arrival Time: Sep 21, 2011 14:02:38.776648000 CEST
    Epoch Time: 1316606558.776648000 seconds
    [Time delta from previous captured frame: 0.000003000 seconds]
    [Time delta from previous displayed frame: 0.000003000 seconds]
    [Time since reference or first frame: 364.309680000 seconds]
    Frame Number: 36
    Frame Length: 64 bytes (512 bits)
    Capture Length: 64 bytes (512 bits)
    [Frame is marked: False]
    [Frame is ignored: False]
    [Protocols in frame: usb:usbhub]
USB URB
    URB id: 0x00000000f37ab080
    URB type: URB_SUBMIT ('S')
    URB transfer type: URB_CONTROL out (0x02)
    Endpoint: 0x80
    Device: 1
    URB bus id: 1
    Device setup request: relevant (0)
    Data: not present ('<')
    URB sec: 1316606558
    URB usec: 776648
    URB status: Operation now in progress (-EINPROGRESS) (-115)
    URB length [bytes]: 4
    Data length [bytes]: 0
    [Response in: 37]
    [bInterfaceClass: Unknown (0xffff)]
    URB setup
        bmRequestType: 0xa3
            1... .... = Direction: Device-to-host
            .01. .... = Type: Class (0x01)
            ...0 0011 = Recipient: Unknown (0x03)
    bRequest: GET_STATUS (0x00)
    wValue: 0x0000
        (zero): 0
    wIndex: 6
        Port: 6
    wLength: 4

0000  80 b0 7a f3 00 00 00 00 53 02 80 01 01 00 00 3c   ..z.....S......<
0010  5e d2 79 4e 00 00 00 00 c8 d9 0b 00 8d ff ff ff   ^.yN............
0020  04 00 00 00 00 00 00 00 a3 00 00 00 06 00 04 00   ................
0030  00 00 00 00 00 00 00 00 00 02 00 00 00 00 00 00   ................

No.     Time        Source                Destination           Protocol Info
     37 364.309685  1.0                   host                  USBHUB   GET_STATUS Response

Frame 37: 68 bytes on wire (544 bits), 68 bytes captured (544 bits)
    Arrival Time: Sep 21, 2011 14:02:38.776653000 CEST
    Epoch Time: 1316606558.776653000 seconds
    [Time delta from previous captured frame: 0.000005000 seconds]
    [Time delta from previous displayed frame: 0.000005000 seconds]
    [Time since reference or first frame: 364.309685000 seconds]
    Frame Number: 37
    Frame Length: 68 bytes (544 bits)
    Capture Length: 68 bytes (544 bits)
    [Frame is marked: False]
    [Frame is ignored: False]
    [Protocols in frame: usb:usbhub]
USB URB
    URB id: 0x00000000f37ab080
    URB type: URB_COMPLETE ('C')
    URB transfer type: URB_CONTROL out (0x02)
    Endpoint: 0x80
    Device: 1
    URB bus id: 1
    Device setup request: not relevant ('-')
    Data: present (0)
    URB sec: 1316606558
    URB usec: 776653
    URB status: Success (0)
    URB length [bytes]: 4
    Data length [bytes]: 4
    [Request in: 36]
    [Time from request: 0.000005000 seconds]
    [bInterfaceClass: Unknown (0xffff)]

0000  80 b0 7a f3 00 00 00 00 43 02 80 01 01 00 2d 00   ..z.....C.....-.
0010  5e d2 79 4e 00 00 00 00 cd d9 0b 00 00 00 00 00   ^.yN............
0020  04 00 00 00 04 00 00 00 00 00 00 00 00 00 00 00   ................
0030  00 00 00 00 00 00 00 00 00 02 00 00 00 00 00 00   ................
0040  00 01 00 00                                       ....

No.     Time        Source                Destination           Protocol Info
     38 364.309688  host                  1.0                   USBHUB   GET_STATUS Request

Frame 38: 64 bytes on wire (512 bits), 64 bytes captured (512 bits)
    Arrival Time: Sep 21, 2011 14:02:38.776656000 CEST
    Epoch Time: 1316606558.776656000 seconds
    [Time delta from previous captured frame: 0.000003000 seconds]
    [Time delta from previous displayed frame: 0.000003000 seconds]
    [Time since reference or first frame: 364.309688000 seconds]
    Frame Number: 38
    Frame Length: 64 bytes (512 bits)
    Capture Length: 64 bytes (512 bits)
    [Frame is marked: False]
    [Frame is ignored: False]
    [Protocols in frame: usb:usbhub]
USB URB
    URB id: 0x00000000f37ab080
    URB type: URB_SUBMIT ('S')
    URB transfer type: URB_CONTROL out (0x02)
    Endpoint: 0x80
    Device: 1
    URB bus id: 1
    Device setup request: relevant (0)
    Data: not present ('<')
    URB sec: 1316606558
    URB usec: 776656
    URB status: Operation now in progress (-EINPROGRESS) (-115)
    URB length [bytes]: 4
    Data length [bytes]: 0
    [Response in: 39]
    [bInterfaceClass: Unknown (0xffff)]
    URB setup
        bmRequestType: 0xa3
            1... .... = Direction: Device-to-host
            .01. .... = Type: Class (0x01)
            ...0 0011 = Recipient: Unknown (0x03)
    bRequest: GET_STATUS (0x00)
    wValue: 0x0000
        (zero): 0
    wIndex: 7
        Port: 7
    wLength: 4

0000  80 b0 7a f3 00 00 00 00 53 02 80 01 01 00 00 3c   ..z.....S......<
0010  5e d2 79 4e 00 00 00 00 d0 d9 0b 00 8d ff ff ff   ^.yN............
0020  04 00 00 00 00 00 00 00 a3 00 00 00 07 00 04 00   ................
0030  00 00 00 00 00 00 00 00 00 02 00 00 00 00 00 00   ................

No.     Time        Source                Destination           Protocol Info
     39 364.309692  1.0                   host                  USBHUB   GET_STATUS Response

Frame 39: 68 bytes on wire (544 bits), 68 bytes captured (544 bits)
    Arrival Time: Sep 21, 2011 14:02:38.776660000 CEST
    Epoch Time: 1316606558.776660000 seconds
    [Time delta from previous captured frame: 0.000004000 seconds]
    [Time delta from previous displayed frame: 0.000004000 seconds]
    [Time since reference or first frame: 364.309692000 seconds]
    Frame Number: 39
    Frame Length: 68 bytes (544 bits)
    Capture Length: 68 bytes (544 bits)
    [Frame is marked: False]
    [Frame is ignored: False]
    [Protocols in frame: usb:usbhub]
USB URB
    URB id: 0x00000000f37ab080
    URB type: URB_COMPLETE ('C')
    URB transfer type: URB_CONTROL out (0x02)
    Endpoint: 0x80
    Device: 1
    URB bus id: 1
    Device setup request: not relevant ('-')
    Data: present (0)
    URB sec: 1316606558
    URB usec: 776660
    URB status: Success (0)
    URB length [bytes]: 4
    Data length [bytes]: 4
    [Request in: 38]
    [Time from request: 0.000004000 seconds]
    [bInterfaceClass: Unknown (0xffff)]

0000  80 b0 7a f3 00 00 00 00 43 02 80 01 01 00 2d 00   ..z.....C.....-.
0010  5e d2 79 4e 00 00 00 00 d4 d9 0b 00 00 00 00 00   ^.yN............
0020  04 00 00 00 04 00 00 00 00 00 00 00 00 00 00 00   ................
0030  00 00 00 00 00 00 00 00 00 02 00 00 00 00 00 00   ................
0040  00 01 00 00                                       ....

No.     Time        Source                Destination           Protocol Info
     40 364.309696  host                  1.0                   USBHUB   GET_STATUS Request

Frame 40: 64 bytes on wire (512 bits), 64 bytes captured (512 bits)
    Arrival Time: Sep 21, 2011 14:02:38.776664000 CEST
    Epoch Time: 1316606558.776664000 seconds
    [Time delta from previous captured frame: 0.000004000 seconds]
    [Time delta from previous displayed frame: 0.000004000 seconds]
    [Time since reference or first frame: 364.309696000 seconds]
    Frame Number: 40
    Frame Length: 64 bytes (512 bits)
    Capture Length: 64 bytes (512 bits)
    [Frame is marked: False]
    [Frame is ignored: False]
    [Protocols in frame: usb:usbhub]
USB URB
    URB id: 0x00000000f37ab080
    URB type: URB_SUBMIT ('S')
    URB transfer type: URB_CONTROL out (0x02)
    Endpoint: 0x80
    Device: 1
    URB bus id: 1
    Device setup request: relevant (0)
    Data: not present ('<')
    URB sec: 1316606558
    URB usec: 776664
    URB status: Operation now in progress (-EINPROGRESS) (-115)
    URB length [bytes]: 4
    Data length [bytes]: 0
    [Response in: 41]
    [bInterfaceClass: Unknown (0xffff)]
    URB setup
        bmRequestType: 0xa3
            1... .... = Direction: Device-to-host
            .01. .... = Type: Class (0x01)
            ...0 0011 = Recipient: Unknown (0x03)
    bRequest: GET_STATUS (0x00)
    wValue: 0x0000
        (zero): 0
    wIndex: 8
        Port: 8
    wLength: 4

0000  80 b0 7a f3 00 00 00 00 53 02 80 01 01 00 00 3c   ..z.....S......<
0010  5e d2 79 4e 00 00 00 00 d8 d9 0b 00 8d ff ff ff   ^.yN............
0020  04 00 00 00 00 00 00 00 a3 00 00 00 08 00 04 00   ................
0030  00 00 00 00 00 00 00 00 00 02 00 00 00 00 00 00   ................

No.     Time        Source                Destination           Protocol Info
     41 364.309700  1.0                   host                  USBHUB   GET_STATUS Response

Frame 41: 68 bytes on wire (544 bits), 68 bytes captured (544 bits)
    Arrival Time: Sep 21, 2011 14:02:38.776668000 CEST
    Epoch Time: 1316606558.776668000 seconds
    [Time delta from previous captured frame: 0.000004000 seconds]
    [Time delta from previous displayed frame: 0.000004000 seconds]
    [Time since reference or first frame: 364.309700000 seconds]
    Frame Number: 41
    Frame Length: 68 bytes (544 bits)
    Capture Length: 68 bytes (544 bits)
    [Frame is marked: False]
    [Frame is ignored: False]
    [Protocols in frame: usb:usbhub]
USB URB
    URB id: 0x00000000f37ab080
    URB type: URB_COMPLETE ('C')
    URB transfer type: URB_CONTROL out (0x02)
    Endpoint: 0x80
    Device: 1
    URB bus id: 1
    Device setup request: not relevant ('-')
    Data: present (0)
    URB sec: 1316606558
    URB usec: 776668
    URB status: Success (0)
    URB length [bytes]: 4
    Data length [bytes]: 4
    [Request in: 40]
    [Time from request: 0.000004000 seconds]
    [bInterfaceClass: Unknown (0xffff)]

0000  80 b0 7a f3 00 00 00 00 43 02 80 01 01 00 2d 00   ..z.....C.....-.
0010  5e d2 79 4e 00 00 00 00 dc d9 0b 00 00 00 00 00   ^.yN............
0020  04 00 00 00 04 00 00 00 00 00 00 00 00 00 00 00   ................
0030  00 00 00 00 00 00 00 00 00 02 00 00 00 00 00 00   ................
0040  00 01 00 00                                       ....

No.     Time        Source                Destination           Protocol Info
     42 364.413654  host                  1.1                   USB      URB_INTERRUPT out

Frame 42: 64 bytes on wire (512 bits), 64 bytes captured (512 bits)
    Arrival Time: Sep 21, 2011 14:02:38.880622000 CEST
    Epoch Time: 1316606558.880622000 seconds
    [Time delta from previous captured frame: 0.103954000 seconds]
    [Time delta from previous displayed frame: 0.103954000 seconds]
    [Time since reference or first frame: 364.413654000 seconds]
    Frame Number: 42
    Frame Length: 64 bytes (512 bits)
    Capture Length: 64 bytes (512 bits)
    [Frame is marked: False]
    [Frame is ignored: False]
    [Protocols in frame: usb]
USB URB
    URB id: 0x00000000f3cecb80
    URB type: URB_SUBMIT ('S')
    URB transfer type: URB_INTERRUPT out (0x01)
    Endpoint: 0x81
    Device: 1
    URB bus id: 1
    Device setup request: not relevant ('-')
    Data: not present ('<')
    URB sec: 1316606558
    URB usec: 880622
    URB status: Operation now in progress (-EINPROGRESS) (-115)
    URB length [bytes]: 4
    Data length [bytes]: 0

0000  80 cb ce f3 00 00 00 00 53 01 81 01 01 00 2d 3c   ........S.....-<
0010  5e d2 79 4e 00 00 00 00 ee 6f 0d 00 8d ff ff ff   ^.yN.....o......
0020  04 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00   ................
0030  00 08 00 00 00 00 00 00 00 02 00 00 00 00 00 00   ................

No.     Time        Source                Destination           Protocol Info
     43 364.413732  host                  1.0                   USBHUB   GET_STATUS Request

Frame 43: 64 bytes on wire (512 bits), 64 bytes captured (512 bits)
    Arrival Time: Sep 21, 2011 14:02:38.880700000 CEST
    Epoch Time: 1316606558.880700000 seconds
    [Time delta from previous captured frame: 0.000078000 seconds]
    [Time delta from previous displayed frame: 0.000078000 seconds]
    [Time since reference or first frame: 364.413732000 seconds]
    Frame Number: 43
    Frame Length: 64 bytes (512 bits)
    Capture Length: 64 bytes (512 bits)
    [Frame is marked: False]
    [Frame is ignored: False]
    [Protocols in frame: usb:usbhub]
USB URB
    URB id: 0x00000000f37ab800
    URB type: URB_SUBMIT ('S')
    URB transfer type: URB_CONTROL out (0x02)
    Endpoint: 0x80
    Device: 1
    URB bus id: 1
    Device setup request: relevant (0)
    Data: not present ('<')
    URB sec: 1316606558
    URB usec: 880700
    URB status: Operation now in progress (-EINPROGRESS) (-115)
    URB length [bytes]: 4
    Data length [bytes]: 0
    [Response in: 44]
    [bInterfaceClass: Unknown (0xffff)]
    URB setup
        bmRequestType: 0xa3
            1... .... = Direction: Device-to-host
            .01. .... = Type: Class (0x01)
            ...0 0011 = Recipient: Unknown (0x03)
    bRequest: GET_STATUS (0x00)
    wValue: 0x0000
        (zero): 0
    wIndex: 5
        Port: 5
    wLength: 4

0000  00 b8 7a f3 00 00 00 00 53 02 80 01 01 00 00 3c   ..z.....S......<
0010  5e d2 79 4e 00 00 00 00 3c 70 0d 00 8d ff ff ff   ^.yN....<p......
0020  04 00 00 00 00 00 00 00 a3 00 00 00 05 00 04 00   ................
0030  00 00 00 00 00 00 00 00 00 02 00 00 00 00 00 00   ................

No.     Time        Source                Destination           Protocol Info
     44 364.413745  1.0                   host                  USBHUB   GET_STATUS Response

Frame 44: 68 bytes on wire (544 bits), 68 bytes captured (544 bits)
    Arrival Time: Sep 21, 2011 14:02:38.880713000 CEST
    Epoch Time: 1316606558.880713000 seconds
    [Time delta from previous captured frame: 0.000013000 seconds]
    [Time delta from previous displayed frame: 0.000013000 seconds]
    [Time since reference or first frame: 364.413745000 seconds]
    Frame Number: 44
    Frame Length: 68 bytes (544 bits)
    Capture Length: 68 bytes (544 bits)
    [Frame is marked: False]
    [Frame is ignored: False]
    [Protocols in frame: usb:usbhub]
USB URB
    URB id: 0x00000000f37ab800
    URB type: URB_COMPLETE ('C')
    URB transfer type: URB_CONTROL out (0x02)
    Endpoint: 0x80
    Device: 1
    URB bus id: 1
    Device setup request: not relevant ('-')
    Data: present (0)
    URB sec: 1316606558
    URB usec: 880713
    URB status: Success (0)
    URB length [bytes]: 4
    Data length [bytes]: 4
    [Request in: 43]
    [Time from request: 0.000013000 seconds]
    [bInterfaceClass: Unknown (0xffff)]

0000  00 b8 7a f3 00 00 00 00 43 02 80 01 01 00 2d 00   ..z.....C.....-.
0010  5e d2 79 4e 00 00 00 00 49 70 0d 00 00 00 00 00   ^.yN....Ip......
0020  04 00 00 00 04 00 00 00 00 00 00 00 00 00 00 00   ................
0030  00 00 00 00 00 00 00 00 00 02 00 00 00 00 00 00   ................
0040  01 05 00 00                                       ....

No.     Time        Source                Destination           Protocol Info
     45 364.413763  host                  1.0                   USBHUB   SET_FEATURE Request

Frame 45: 64 bytes on wire (512 bits), 64 bytes captured (512 bits)
    Arrival Time: Sep 21, 2011 14:02:38.880731000 CEST
    Epoch Time: 1316606558.880731000 seconds
    [Time delta from previous captured frame: 0.000018000 seconds]
    [Time delta from previous displayed frame: 0.000018000 seconds]
    [Time since reference or first frame: 364.413763000 seconds]
    Frame Number: 45
    Frame Length: 64 bytes (512 bits)
    Capture Length: 64 bytes (512 bits)
    [Frame is marked: False]
    [Frame is ignored: False]
    [Protocols in frame: usb:usbhub]
USB URB
    URB id: 0x00000000f37ab800
    URB type: URB_SUBMIT ('S')
    URB transfer type: URB_CONTROL out (0x02)
    Endpoint: 0x00
    Device: 1
    URB bus id: 1
    Device setup request: relevant (0)
    Data: present (0)
    URB sec: 1316606558
    URB usec: 880731
    URB status: Operation now in progress (-EINPROGRESS) (-115)
    URB length [bytes]: 0
    Data length [bytes]: 0
    [Response in: 46]
    [bInterfaceClass: Unknown (0xffff)]
    URB setup
        bmRequestType: 0x23
            0... .... = Direction: Host-to-device
            .01. .... = Type: Class (0x01)
            ...0 0011 = Recipient: Unknown (0x03)
    bRequest: SET_FEATURE (0x03)
    wValue: 0x0004
        PortFeatureSelector: PORT_RESET (4)
    wIndex: 5
        Port: 5
        PortSelector: 0
    wLength: 0
        (zero): 0

0000  00 b8 7a f3 00 00 00 00 53 02 00 01 01 00 00 00   ..z.....S.......
0010  5e d2 79 4e 00 00 00 00 5b 70 0d 00 8d ff ff ff   ^.yN....[p......
0020  00 00 00 00 00 00 00 00 23 03 04 00 05 00 00 00   ........#.......
0030  00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00   ................

No.     Time        Source                Destination           Protocol Info
     46 364.413770  1.0                   host                  USBHUB   SET_FEATURE Response

Frame 46: 64 bytes on wire (512 bits), 64 bytes captured (512 bits)
    Arrival Time: Sep 21, 2011 14:02:38.880738000 CEST
    Epoch Time: 1316606558.880738000 seconds
    [Time delta from previous captured frame: 0.000007000 seconds]
    [Time delta from previous displayed frame: 0.000007000 seconds]
    [Time since reference or first frame: 364.413770000 seconds]
    Frame Number: 46
    Frame Length: 64 bytes (512 bits)
    Capture Length: 64 bytes (512 bits)
    [Frame is marked: False]
    [Frame is ignored: False]
    [Protocols in frame: usb:usbhub]
USB URB
    URB id: 0x00000000f37ab800
    URB type: URB_COMPLETE ('C')
    URB transfer type: URB_CONTROL out (0x02)
    Endpoint: 0x00
    Device: 1
    URB bus id: 1
    Device setup request: not relevant ('-')
    Data: not present ('>')
    URB sec: 1316606558
    URB usec: 880738
    URB status: Success (0)
    URB length [bytes]: 0
    Data length [bytes]: 0
    [Request in: 45]
    [Time from request: 0.000007000 seconds]
    [bInterfaceClass: Unknown (0xffff)]

0000  00 b8 7a f3 00 00 00 00 43 02 00 01 01 00 2d 3e   ..z.....C.....->
0010  5e d2 79 4e 00 00 00 00 62 70 0d 00 00 00 00 00   ^.yN....bp......
0020  00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00   ................
0030  00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00   ................

No.     Time        Source                Destination           Protocol Info
     47 364.469605  host                  1.0                   USBHUB   GET_STATUS Request

Frame 47: 64 bytes on wire (512 bits), 64 bytes captured (512 bits)
    Arrival Time: Sep 21, 2011 14:02:38.936573000 CEST
    Epoch Time: 1316606558.936573000 seconds
    [Time delta from previous captured frame: 0.055835000 seconds]
    [Time delta from previous displayed frame: 0.055835000 seconds]
    [Time since reference or first frame: 364.469605000 seconds]
    Frame Number: 47
    Frame Length: 64 bytes (512 bits)
    Capture Length: 64 bytes (512 bits)
    [Frame is marked: False]
    [Frame is ignored: False]
    [Protocols in frame: usb:usbhub]
USB URB
    URB id: 0x00000000f37ab800
    URB type: URB_SUBMIT ('S')
    URB transfer type: URB_CONTROL out (0x02)
    Endpoint: 0x80
    Device: 1
    URB bus id: 1
    Device setup request: relevant (0)
    Data: not present ('<')
    URB sec: 1316606558
    URB usec: 936573
    URB status: Operation now in progress (-EINPROGRESS) (-115)
    URB length [bytes]: 4
    Data length [bytes]: 0
    [Response in: 48]
    [bInterfaceClass: Unknown (0xffff)]
    URB setup
        bmRequestType: 0xa3
            1... .... = Direction: Device-to-host
            .01. .... = Type: Class (0x01)
            ...0 0011 = Recipient: Unknown (0x03)
    bRequest: GET_STATUS (0x00)
    wValue: 0x0000
        (zero): 0
    wIndex: 5
        Port: 5
    wLength: 4

0000  00 b8 7a f3 00 00 00 00 53 02 80 01 01 00 00 3c   ..z.....S......<
0010  5e d2 79 4e 00 00 00 00 7d 4a 0e 00 8d ff ff ff   ^.yN....}J......
0020  04 00 00 00 00 00 00 00 a3 00 00 00 05 00 04 00   ................
0030  00 00 00 00 00 00 00 00 00 02 00 00 00 00 00 00   ................

No.     Time        Source                Destination           Protocol Info
     48 364.469829  1.0                   host                  USBHUB   GET_STATUS Response

Frame 48: 68 bytes on wire (544 bits), 68 bytes captured (544 bits)
    Arrival Time: Sep 21, 2011 14:02:38.936797000 CEST
    Epoch Time: 1316606558.936797000 seconds
    [Time delta from previous captured frame: 0.000224000 seconds]
    [Time delta from previous displayed frame: 0.000224000 seconds]
    [Time since reference or first frame: 364.469829000 seconds]
    Frame Number: 48
    Frame Length: 68 bytes (544 bits)
    Capture Length: 68 bytes (544 bits)
    [Frame is marked: False]
    [Frame is ignored: False]
    [Protocols in frame: usb:usbhub]
USB URB
    URB id: 0x00000000f37ab800
    URB type: URB_COMPLETE ('C')
    URB transfer type: URB_CONTROL out (0x02)
    Endpoint: 0x80
    Device: 1
    URB bus id: 1
    Device setup request: not relevant ('-')
    Data: present (0)
    URB sec: 1316606558
    URB usec: 936797
    URB status: Success (0)
    URB length [bytes]: 4
    Data length [bytes]: 4
    [Request in: 47]
    [Time from request: 0.000224000 seconds]
    [bInterfaceClass: Unknown (0xffff)]

0000  00 b8 7a f3 00 00 00 00 43 02 80 01 01 00 2d 00   ..z.....C.....-.
0010  5e d2 79 4e 00 00 00 00 5d 4b 0e 00 00 00 00 00   ^.yN....]K......
0020  04 00 00 00 04 00 00 00 00 00 00 00 00 00 00 00   ................
0030  00 00 00 00 00 00 00 00 00 02 00 00 00 00 00 00   ................
0040  03 05 10 00                                       ....

No.     Time        Source                Destination           Protocol Info
     49 364.525672  host                  1.0                   USBHUB   CLEAR_FEATURE Request

Frame 49: 64 bytes on wire (512 bits), 64 bytes captured (512 bits)
    Arrival Time: Sep 21, 2011 14:02:38.992640000 CEST
    Epoch Time: 1316606558.992640000 seconds
    [Time delta from previous captured frame: 0.055843000 seconds]
    [Time delta from previous displayed frame: 0.055843000 seconds]
    [Time since reference or first frame: 364.525672000 seconds]
    Frame Number: 49
    Frame Length: 64 bytes (512 bits)
    Capture Length: 64 bytes (512 bits)
    [Frame is marked: False]
    [Frame is ignored: False]
    [Protocols in frame: usb:usbhub]
USB URB
    URB id: 0x00000000f37ab800
    URB type: URB_SUBMIT ('S')
    URB transfer type: URB_CONTROL out (0x02)
    Endpoint: 0x00
    Device: 1
    URB bus id: 1
    Device setup request: relevant (0)
    Data: present (0)
    URB sec: 1316606558
    URB usec: 992640
    URB status: Operation now in progress (-EINPROGRESS) (-115)
    URB length [bytes]: 0
    Data length [bytes]: 0
    [Response in: 50]
    [bInterfaceClass: Unknown (0xffff)]
    URB setup
        bmRequestType: 0x23
            0... .... = Direction: Host-to-device
            .01. .... = Type: Class (0x01)
            ...0 0011 = Recipient: Unknown (0x03)
    bRequest: CLEAR_FEATURE (0x01)
    wValue: 0x0014
        PortFeatureSelector: C_PORT_RESET (20)
    wIndex: 5
        Port: 5
        PortSelector: 0
    wLength: 0
        (zero): 0

0000  00 b8 7a f3 00 00 00 00 53 02 00 01 01 00 00 00   ..z.....S.......
0010  5e d2 79 4e 00 00 00 00 80 25 0f 00 8d ff ff ff   ^.yN.....%......
0020  00 00 00 00 00 00 00 00 23 01 14 00 05 00 00 00   ........#.......
0030  00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00   ................

No.     Time        Source                Destination           Protocol Info
     50 364.525689  1.0                   host                  USBHUB   CLEAR_FEATURE Response

Frame 50: 64 bytes on wire (512 bits), 64 bytes captured (512 bits)
    Arrival Time: Sep 21, 2011 14:02:38.992657000 CEST
    Epoch Time: 1316606558.992657000 seconds
    [Time delta from previous captured frame: 0.000017000 seconds]
    [Time delta from previous displayed frame: 0.000017000 seconds]
    [Time since reference or first frame: 364.525689000 seconds]
    Frame Number: 50
    Frame Length: 64 bytes (512 bits)
    Capture Length: 64 bytes (512 bits)
    [Frame is marked: False]
    [Frame is ignored: False]
    [Protocols in frame: usb:usbhub]
USB URB
    URB id: 0x00000000f37ab800
    URB type: URB_COMPLETE ('C')
    URB transfer type: URB_CONTROL out (0x02)
    Endpoint: 0x00
    Device: 1
    URB bus id: 1
    Device setup request: not relevant ('-')
    Data: not present ('>')
    URB sec: 1316606558
    URB usec: 992657
    URB status: Success (0)
    URB length [bytes]: 0
    Data length [bytes]: 0
    [Request in: 49]
    [Time from request: 0.000017000 seconds]
    [bInterfaceClass: Unknown (0xffff)]

0000  00 b8 7a f3 00 00 00 00 43 02 00 01 01 00 2d 3e   ..z.....C.....->
0010  5e d2 79 4e 00 00 00 00 91 25 0f 00 00 00 00 00   ^.yN.....%......
0020  00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00   ................
0030  00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00   ................

No.     Time        Source                Destination           Protocol Info
     51 364.525712  host                  0.0                   USB      GET DESCRIPTOR Request DEVICE

Frame 51: 64 bytes on wire (512 bits), 64 bytes captured (512 bits)
    Arrival Time: Sep 21, 2011 14:02:38.992680000 CEST
    Epoch Time: 1316606558.992680000 seconds
    [Time delta from previous captured frame: 0.000023000 seconds]
    [Time delta from previous displayed frame: 0.000023000 seconds]
    [Time since reference or first frame: 364.525712000 seconds]
    Frame Number: 51
    Frame Length: 64 bytes (512 bits)
    Capture Length: 64 bytes (512 bits)
    [Frame is marked: False]
    [Frame is ignored: False]
    [Protocols in frame: usb]
USB URB
    URB id: 0x00000000f37ab800
    URB type: URB_SUBMIT ('S')
    URB transfer type: URB_CONTROL out (0x02)
    Endpoint: 0x80
    Device: 0
    URB bus id: 1
    Device setup request: relevant (0)
    Data: not present ('<')
    URB sec: 1316606558
    URB usec: 992680
    URB status: Operation now in progress (-EINPROGRESS) (-115)
    URB length [bytes]: 64
    Data length [bytes]: 0
    [Response in: 52]
    [bInterfaceClass: Unknown (0xffff)]
    URB setup
        bmRequestType: 0x80
            1... .... = Direction: Device-to-host
            .00. .... = Type: Standard (0x00)
            ...0 0000 = Recipient: Device (0x00)
        bRequest: GET DESCRIPTOR (6)
        Descriptor Index: 0x00
        bDescriptorType: DEVICE (1)
        Language Id: no language specified (0x0000)
        wLength: 64

0000  00 b8 7a f3 00 00 00 00 53 02 80 00 01 00 00 3c   ..z.....S......<
0010  5e d2 79 4e 00 00 00 00 a8 25 0f 00 8d ff ff ff   ^.yN.....%......
0020  40 00 00 00 00 00 00 00 80 06 00 01 00 00 40 00   @.............@.
0030  00 00 00 00 00 00 00 00 00 02 00 00 00 00 00 00   ................

No.     Time        Source                Destination           Protocol Info
     52 364.526475  0.0                   host                  USB      GET DESCRIPTOR Response DEVICE

Frame 52: 82 bytes on wire (656 bits), 82 bytes captured (656 bits)
    Arrival Time: Sep 21, 2011 14:02:38.993443000 CEST
    Epoch Time: 1316606558.993443000 seconds
    [Time delta from previous captured frame: 0.000763000 seconds]
    [Time delta from previous displayed frame: 0.000763000 seconds]
    [Time since reference or first frame: 364.526475000 seconds]
    Frame Number: 52
    Frame Length: 82 bytes (656 bits)
    Capture Length: 82 bytes (656 bits)
    [Frame is marked: False]
    [Frame is ignored: False]
    [Protocols in frame: usb]
USB URB
    URB id: 0x00000000f37ab800
    URB type: URB_COMPLETE ('C')
    URB transfer type: URB_CONTROL out (0x02)
    Endpoint: 0x80
    Device: 0
    URB bus id: 1
    Device setup request: not relevant ('-')
    Data: present (0)
    URB sec: 1316606558
    URB usec: 993443
    URB status: Success (0)
    URB length [bytes]: 18
    Data length [bytes]: 18
    [Request in: 51]
    [Time from request: 0.000763000 seconds]
    [bInterfaceClass: Unknown (0xffff)]
    DEVICE DESCRIPTOR
        bLength: 18
        bDescriptorType: DEVICE (1)
        bcdUSB: 0x0200
        bDeviceClass: 0
        bDeviceSubClass: 0
        bDeviceProtocol: 0
        bMaxPacketSize0: 64
        idVendor: 0x132b
        idProduct: 0x20b8
        bcdDevice: 0x0100
        iManufacturer: 1
        iProduct: 2
        iSerialNumber: 0
        bNumConfigurations: 1

0000  00 b8 7a f3 00 00 00 00 43 02 80 00 01 00 2d 00   ..z.....C.....-.
0010  5e d2 79 4e 00 00 00 00 a3 28 0f 00 00 00 00 00   ^.yN.....(......
0020  12 00 00 00 12 00 00 00 00 00 00 00 00 00 00 00   ................
0030  00 00 00 00 00 00 00 00 00 02 00 00 00 00 00 00   ................
0040  12 01 00 02 00 00 00 40 2b 13 b8 20 00 01 01 02   .......@+.. ....
0050  00 01                                             ..

No.     Time        Source                Destination           Protocol Info
     53 364.526520  host                  1.0                   USBHUB   SET_FEATURE Request

Frame 53: 64 bytes on wire (512 bits), 64 bytes captured (512 bits)
    Arrival Time: Sep 21, 2011 14:02:38.993488000 CEST
    Epoch Time: 1316606558.993488000 seconds
    [Time delta from previous captured frame: 0.000045000 seconds]
    [Time delta from previous displayed frame: 0.000045000 seconds]
    [Time since reference or first frame: 364.526520000 seconds]
    Frame Number: 53
    Frame Length: 64 bytes (512 bits)
    Capture Length: 64 bytes (512 bits)
    [Frame is marked: False]
    [Frame is ignored: False]
    [Protocols in frame: usb:usbhub]
USB URB
    URB id: 0x00000000f37ab800
    URB type: URB_SUBMIT ('S')
    URB transfer type: URB_CONTROL out (0x02)
    Endpoint: 0x00
    Device: 1
    URB bus id: 1
    Device setup request: relevant (0)
    Data: present (0)
    URB sec: 1316606558
    URB usec: 993488
    URB status: Operation now in progress (-EINPROGRESS) (-115)
    URB length [bytes]: 0
    Data length [bytes]: 0
    [Response in: 54]
    [bInterfaceClass: Unknown (0xffff)]
    URB setup
        bmRequestType: 0x23
            0... .... = Direction: Host-to-device
            .01. .... = Type: Class (0x01)
            ...0 0011 = Recipient: Unknown (0x03)
    bRequest: SET_FEATURE (0x03)
    wValue: 0x0004
        PortFeatureSelector: PORT_RESET (4)
    wIndex: 5
        Port: 5
        PortSelector: 0
    wLength: 0
        (zero): 0

0000  00 b8 7a f3 00 00 00 00 53 02 00 01 01 00 00 00   ..z.....S.......
0010  5e d2 79 4e 00 00 00 00 d0 28 0f 00 8d ff ff ff   ^.yN.....(......
0020  00 00 00 00 00 00 00 00 23 03 04 00 05 00 00 00   ........#.......
0030  00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00   ................

No.     Time        Source                Destination           Protocol Info
     54 364.526531  1.0                   host                  USBHUB   SET_FEATURE Response

Frame 54: 64 bytes on wire (512 bits), 64 bytes captured (512 bits)
    Arrival Time: Sep 21, 2011 14:02:38.993499000 CEST
    Epoch Time: 1316606558.993499000 seconds
    [Time delta from previous captured frame: 0.000011000 seconds]
    [Time delta from previous displayed frame: 0.000011000 seconds]
    [Time since reference or first frame: 364.526531000 seconds]
    Frame Number: 54
    Frame Length: 64 bytes (512 bits)
    Capture Length: 64 bytes (512 bits)
    [Frame is marked: False]
    [Frame is ignored: False]
    [Protocols in frame: usb:usbhub]
USB URB
    URB id: 0x00000000f37ab800
    URB type: URB_COMPLETE ('C')
    URB transfer type: URB_CONTROL out (0x02)
    Endpoint: 0x00
    Device: 1
    URB bus id: 1
    Device setup request: not relevant ('-')
    Data: not present ('>')
    URB sec: 1316606558
    URB usec: 993499
    URB status: Success (0)
    URB length [bytes]: 0
    Data length [bytes]: 0
    [Request in: 53]
    [Time from request: 0.000011000 seconds]
    [bInterfaceClass: Unknown (0xffff)]

0000  00 b8 7a f3 00 00 00 00 43 02 00 01 01 00 2d 3e   ..z.....C.....->
0010  5e d2 79 4e 00 00 00 00 db 28 0f 00 00 00 00 00   ^.yN.....(......
0020  00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00   ................
0030  00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00   ................

No.     Time        Source                Destination           Protocol Info
     55 364.581610  host                  1.0                   USBHUB   GET_STATUS Request

Frame 55: 64 bytes on wire (512 bits), 64 bytes captured (512 bits)
    Arrival Time: Sep 21, 2011 14:02:39.048578000 CEST
    Epoch Time: 1316606559.048578000 seconds
    [Time delta from previous captured frame: 0.055079000 seconds]
    [Time delta from previous displayed frame: 0.055079000 seconds]
    [Time since reference or first frame: 364.581610000 seconds]
    Frame Number: 55
    Frame Length: 64 bytes (512 bits)
    Capture Length: 64 bytes (512 bits)
    [Frame is marked: False]
    [Frame is ignored: False]
    [Protocols in frame: usb:usbhub]
USB URB
    URB id: 0x00000000f37abd00
    URB type: URB_SUBMIT ('S')
    URB transfer type: URB_CONTROL out (0x02)
    Endpoint: 0x80
    Device: 1
    URB bus id: 1
    Device setup request: relevant (0)
    Data: not present ('<')
    URB sec: 1316606559
    URB usec: 48578
    URB status: Operation now in progress (-EINPROGRESS) (-115)
    URB length [bytes]: 4
    Data length [bytes]: 0
    [Response in: 56]
    [bInterfaceClass: Unknown (0xffff)]
    URB setup
        bmRequestType: 0xa3
            1... .... = Direction: Device-to-host
            .01. .... = Type: Class (0x01)
            ...0 0011 = Recipient: Unknown (0x03)
    bRequest: GET_STATUS (0x00)
    wValue: 0x0000
        (zero): 0
    wIndex: 5
        Port: 5
    wLength: 4

0000  00 bd 7a f3 00 00 00 00 53 02 80 01 01 00 00 3c   ..z.....S......<
0010  5f d2 79 4e 00 00 00 00 c2 bd 00 00 8d ff ff ff   _.yN............
0020  04 00 00 00 00 00 00 00 a3 00 00 00 05 00 04 00   ................
0030  00 00 00 00 00 00 00 00 00 02 00 00 00 00 00 00   ................

No.     Time        Source                Destination           Protocol Info
     56 364.581838  1.0                   host                  USBHUB   GET_STATUS Response

Frame 56: 68 bytes on wire (544 bits), 68 bytes captured (544 bits)
    Arrival Time: Sep 21, 2011 14:02:39.048806000 CEST
    Epoch Time: 1316606559.048806000 seconds
    [Time delta from previous captured frame: 0.000228000 seconds]
    [Time delta from previous displayed frame: 0.000228000 seconds]
    [Time since reference or first frame: 364.581838000 seconds]
    Frame Number: 56
    Frame Length: 68 bytes (544 bits)
    Capture Length: 68 bytes (544 bits)
    [Frame is marked: False]
    [Frame is ignored: False]
    [Protocols in frame: usb:usbhub]
USB URB
    URB id: 0x00000000f37abd00
    URB type: URB_COMPLETE ('C')
    URB transfer type: URB_CONTROL out (0x02)
    Endpoint: 0x80
    Device: 1
    URB bus id: 1
    Device setup request: not relevant ('-')
    Data: present (0)
    URB sec: 1316606559
    URB usec: 48806
    URB status: Success (0)
    URB length [bytes]: 4
    Data length [bytes]: 4
    [Request in: 55]
    [Time from request: 0.000228000 seconds]
    [bInterfaceClass: Unknown (0xffff)]

0000  00 bd 7a f3 00 00 00 00 43 02 80 01 01 00 2d 00   ..z.....C.....-.
0010  5f d2 79 4e 00 00 00 00 a6 be 00 00 00 00 00 00   _.yN............
0020  04 00 00 00 04 00 00 00 00 00 00 00 00 00 00 00   ................
0030  00 00 00 00 00 00 00 00 00 02 00 00 00 00 00 00   ................
0040  03 05 10 00                                       ....

No.     Time        Source                Destination           Protocol Info
     57 364.637593  host                  1.0                   USBHUB   CLEAR_FEATURE Request

Frame 57: 64 bytes on wire (512 bits), 64 bytes captured (512 bits)
    Arrival Time: Sep 21, 2011 14:02:39.104561000 CEST
    Epoch Time: 1316606559.104561000 seconds
    [Time delta from previous captured frame: 0.055755000 seconds]
    [Time delta from previous displayed frame: 0.055755000 seconds]
    [Time since reference or first frame: 364.637593000 seconds]
    Frame Number: 57
    Frame Length: 64 bytes (512 bits)
    Capture Length: 64 bytes (512 bits)
    [Frame is marked: False]
    [Frame is ignored: False]
    [Protocols in frame: usb:usbhub]
USB URB
    URB id: 0x00000000f37abb00
    URB type: URB_SUBMIT ('S')
    URB transfer type: URB_CONTROL out (0x02)
    Endpoint: 0x00
    Device: 1
    URB bus id: 1
    Device setup request: relevant (0)
    Data: present (0)
    URB sec: 1316606559
    URB usec: 104561
    URB status: Operation now in progress (-EINPROGRESS) (-115)
    URB length [bytes]: 0
    Data length [bytes]: 0
    [Response in: 58]
    [bInterfaceClass: Unknown (0xffff)]
    URB setup
        bmRequestType: 0x23
            0... .... = Direction: Host-to-device
            .01. .... = Type: Class (0x01)
            ...0 0011 = Recipient: Unknown (0x03)
    bRequest: CLEAR_FEATURE (0x01)
    wValue: 0x0014
        PortFeatureSelector: C_PORT_RESET (20)
    wIndex: 5
        Port: 5
        PortSelector: 0
    wLength: 0
        (zero): 0

0000  00 bb 7a f3 00 00 00 00 53 02 00 01 01 00 00 00   ..z.....S.......
0010  5f d2 79 4e 00 00 00 00 71 98 01 00 8d ff ff ff   _.yN....q.......
0020  00 00 00 00 00 00 00 00 23 01 14 00 05 00 00 00   ........#.......
0030  00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00   ................

No.     Time        Source                Destination           Protocol Info
     58 364.637610  1.0                   host                  USBHUB   CLEAR_FEATURE Response

Frame 58: 64 bytes on wire (512 bits), 64 bytes captured (512 bits)
    Arrival Time: Sep 21, 2011 14:02:39.104578000 CEST
    Epoch Time: 1316606559.104578000 seconds
    [Time delta from previous captured frame: 0.000017000 seconds]
    [Time delta from previous displayed frame: 0.000017000 seconds]
    [Time since reference or first frame: 364.637610000 seconds]
    Frame Number: 58
    Frame Length: 64 bytes (512 bits)
    Capture Length: 64 bytes (512 bits)
    [Frame is marked: False]
    [Frame is ignored: False]
    [Protocols in frame: usb:usbhub]
USB URB
    URB id: 0x00000000f37abb00
    URB type: URB_COMPLETE ('C')
    URB transfer type: URB_CONTROL out (0x02)
    Endpoint: 0x00
    Device: 1
    URB bus id: 1
    Device setup request: not relevant ('-')
    Data: not present ('>')
    URB sec: 1316606559
    URB usec: 104578
    URB status: Success (0)
    URB length [bytes]: 0
    Data length [bytes]: 0
    [Request in: 57]
    [Time from request: 0.000017000 seconds]
    [bInterfaceClass: Unknown (0xffff)]

0000  00 bb 7a f3 00 00 00 00 43 02 00 01 01 00 2d 3e   ..z.....C.....->
0010  5f d2 79 4e 00 00 00 00 82 98 01 00 00 00 00 00   _.yN............
0020  00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00   ................
0030  00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00   ................

No.     Time        Source                Destination           Protocol Info
     59 364.637618  host                  0.0                   USB      SET ADDRESS Request

Frame 59: 64 bytes on wire (512 bits), 64 bytes captured (512 bits)
    Arrival Time: Sep 21, 2011 14:02:39.104586000 CEST
    Epoch Time: 1316606559.104586000 seconds
    [Time delta from previous captured frame: 0.000008000 seconds]
    [Time delta from previous displayed frame: 0.000008000 seconds]
    [Time since reference or first frame: 364.637618000 seconds]
    Frame Number: 59
    Frame Length: 64 bytes (512 bits)
    Capture Length: 64 bytes (512 bits)
    [Frame is marked: False]
    [Frame is ignored: False]
    [Protocols in frame: usb]
USB URB
    URB id: 0x00000000f37abb00
    URB type: URB_SUBMIT ('S')
    URB transfer type: URB_CONTROL out (0x02)
    Endpoint: 0x00
    Device: 0
    URB bus id: 1
    Device setup request: relevant (0)
    Data: present (0)
    URB sec: 1316606559
    URB usec: 104586
    URB status: Operation now in progress (-EINPROGRESS) (-115)
    URB length [bytes]: 0
    Data length [bytes]: 0
    [Response in: 60]
    [bInterfaceClass: Unknown (0xffff)]
    URB setup
        bmRequestType: 0x00
            0... .... = Direction: Host-to-device
            .00. .... = Type: Standard (0x00)
            ...0 0000 = Recipient: Device (0x00)
        bRequest: SET ADDRESS (5)
        Device: 4
        wIndex: 0
        wLength: 0

0000  00 bb 7a f3 00 00 00 00 53 02 00 00 01 00 00 00   ..z.....S.......
0010  5f d2 79 4e 00 00 00 00 8a 98 01 00 8d ff ff ff   _.yN............
0020  00 00 00 00 00 00 00 00 00 05 04 00 00 00 00 00   ................
0030  00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00   ................

No.     Time        Source                Destination           Protocol Info
     60 364.637734  0.0                   host                  USB      SET ADDRESS Response

Frame 60: 64 bytes on wire (512 bits), 64 bytes captured (512 bits)
    Arrival Time: Sep 21, 2011 14:02:39.104702000 CEST
    Epoch Time: 1316606559.104702000 seconds
    [Time delta from previous captured frame: 0.000116000 seconds]
    [Time delta from previous displayed frame: 0.000116000 seconds]
    [Time since reference or first frame: 364.637734000 seconds]
    Frame Number: 60
    Frame Length: 64 bytes (512 bits)
    Capture Length: 64 bytes (512 bits)
    [Frame is marked: False]
    [Frame is ignored: False]
    [Protocols in frame: usb]
USB URB
    URB id: 0x00000000f37abb00
    URB type: URB_COMPLETE ('C')
    URB transfer type: URB_CONTROL out (0x02)
    Endpoint: 0x00
    Device: 0
    URB bus id: 1
    Device setup request: not relevant ('-')
    Data: not present ('>')
    URB sec: 1316606559
    URB usec: 104702
    URB status: Success (0)
    URB length [bytes]: 0
    Data length [bytes]: 0
    [Request in: 59]
    [Time from request: 0.000116000 seconds]
    [bInterfaceClass: Unknown (0xffff)]

0000  00 bb 7a f3 00 00 00 00 43 02 00 00 01 00 2d 3e   ..z.....C.....->
0010  5f d2 79 4e 00 00 00 00 fe 98 01 00 00 00 00 00   _.yN............
0020  00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00   ................
0030  00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00   ................

No.     Time        Source                Destination           Protocol Info
     61 364.657597  host                  4.0                   USB      GET DESCRIPTOR Request DEVICE

Frame 61: 64 bytes on wire (512 bits), 64 bytes captured (512 bits)
    Arrival Time: Sep 21, 2011 14:02:39.124565000 CEST
    Epoch Time: 1316606559.124565000 seconds
    [Time delta from previous captured frame: 0.019863000 seconds]
    [Time delta from previous displayed frame: 0.019863000 seconds]
    [Time since reference or first frame: 364.657597000 seconds]
    Frame Number: 61
    Frame Length: 64 bytes (512 bits)
    Capture Length: 64 bytes (512 bits)
    [Frame is marked: False]
    [Frame is ignored: False]
    [Protocols in frame: usb]
USB URB
    URB id: 0x00000000f37abb00
    URB type: URB_SUBMIT ('S')
    URB transfer type: URB_CONTROL out (0x02)
    Endpoint: 0x80
    Device: 4
    URB bus id: 1
    Device setup request: relevant (0)
    Data: not present ('<')
    URB sec: 1316606559
    URB usec: 124565
    URB status: Operation now in progress (-EINPROGRESS) (-115)
    URB length [bytes]: 18
    Data length [bytes]: 0
    [Response in: 62]
    [bInterfaceClass: PRINTER (0x07)]
    URB setup
        bmRequestType: 0x80
            1... .... = Direction: Device-to-host
            .00. .... = Type: Standard (0x00)
            ...0 0000 = Recipient: Device (0x00)
        bRequest: GET DESCRIPTOR (6)
        Descriptor Index: 0x00
        bDescriptorType: DEVICE (1)
        Language Id: no language specified (0x0000)
        wLength: 18

0000  00 bb 7a f3 00 00 00 00 53 02 80 04 01 00 00 3c   ..z.....S......<
0010  5f d2 79 4e 00 00 00 00 95 e6 01 00 8d ff ff ff   _.yN............
0020  12 00 00 00 00 00 00 00 80 06 00 01 00 00 12 00   ................
0030  00 00 00 00 00 00 00 00 00 02 00 00 00 00 00 00   ................

No.     Time        Source                Destination           Protocol Info
     62 364.657735  4.0                   host                  USB      GET DESCRIPTOR Response DEVICE

Frame 62: 82 bytes on wire (656 bits), 82 bytes captured (656 bits)
    Arrival Time: Sep 21, 2011 14:02:39.124703000 CEST
    Epoch Time: 1316606559.124703000 seconds
    [Time delta from previous captured frame: 0.000138000 seconds]
    [Time delta from previous displayed frame: 0.000138000 seconds]
    [Time since reference or first frame: 364.657735000 seconds]
    Frame Number: 62
    Frame Length: 82 bytes (656 bits)
    Capture Length: 82 bytes (656 bits)
    [Frame is marked: False]
    [Frame is ignored: False]
    [Protocols in frame: usb]
USB URB
    URB id: 0x00000000f37abb00
    URB type: URB_COMPLETE ('C')
    URB transfer type: URB_CONTROL out (0x02)
    Endpoint: 0x80
    Device: 4
    URB bus id: 1
    Device setup request: not relevant ('-')
    Data: present (0)
    URB sec: 1316606559
    URB usec: 124703
    URB status: Success (0)
    URB length [bytes]: 18
    Data length [bytes]: 18
    [Request in: 61]
    [Time from request: 0.000138000 seconds]
    [bInterfaceClass: PRINTER (0x07)]
    DEVICE DESCRIPTOR
        bLength: 18
        bDescriptorType: DEVICE (1)
        bcdUSB: 0x0200
        bDeviceClass: 0
        bDeviceSubClass: 0
        bDeviceProtocol: 0
        bMaxPacketSize0: 64
        idVendor: 0x132b
        idProduct: 0x20b8
        bcdDevice: 0x0100
        iManufacturer: 1
        iProduct: 2
        iSerialNumber: 0
        bNumConfigurations: 1

0000  00 bb 7a f3 00 00 00 00 43 02 80 04 01 00 2d 00   ..z.....C.....-.
0010  5f d2 79 4e 00 00 00 00 1f e7 01 00 00 00 00 00   _.yN............
0020  12 00 00 00 12 00 00 00 00 00 00 00 00 00 00 00   ................
0030  00 00 00 00 00 00 00 00 00 02 00 00 00 00 00 00   ................
0040  12 01 00 02 00 00 00 40 2b 13 b8 20 00 01 01 02   .......@+.. ....
0050  00 01                                             ..

No.     Time        Source                Destination           Protocol Info
     63 364.657788  host                  4.0                   USB      GET DESCRIPTOR Request CONFIGURATION

Frame 63: 64 bytes on wire (512 bits), 64 bytes captured (512 bits)
    Arrival Time: Sep 21, 2011 14:02:39.124756000 CEST
    Epoch Time: 1316606559.124756000 seconds
    [Time delta from previous captured frame: 0.000053000 seconds]
    [Time delta from previous displayed frame: 0.000053000 seconds]
    [Time since reference or first frame: 364.657788000 seconds]
    Frame Number: 63
    Frame Length: 64 bytes (512 bits)
    Capture Length: 64 bytes (512 bits)
    [Frame is marked: False]
    [Frame is ignored: False]
    [Protocols in frame: usb]
USB URB
    URB id: 0x00000000f37abb00
    URB type: URB_SUBMIT ('S')
    URB transfer type: URB_CONTROL out (0x02)
    Endpoint: 0x80
    Device: 4
    URB bus id: 1
    Device setup request: relevant (0)
    Data: not present ('<')
    URB sec: 1316606559
    URB usec: 124756
    URB status: Operation now in progress (-EINPROGRESS) (-115)
    URB length [bytes]: 9
    Data length [bytes]: 0
    [Response in: 64]
    [bInterfaceClass: PRINTER (0x07)]
    URB setup
        bmRequestType: 0x80
            1... .... = Direction: Device-to-host
            .00. .... = Type: Standard (0x00)
            ...0 0000 = Recipient: Device (0x00)
        bRequest: GET DESCRIPTOR (6)
        Descriptor Index: 0x00
        bDescriptorType: CONFIGURATION (2)
        Language Id: no language specified (0x0000)
        wLength: 9

0000  00 bb 7a f3 00 00 00 00 53 02 80 04 01 00 00 3c   ..z.....S......<
0010  5f d2 79 4e 00 00 00 00 54 e7 01 00 8d ff ff ff   _.yN....T.......
0020  09 00 00 00 00 00 00 00 80 06 00 02 00 00 09 00   ................
0030  00 00 00 00 00 00 00 00 00 02 00 00 00 00 00 00   ................

No.     Time        Source                Destination           Protocol Info
     64 364.658109  4.0                   host                  USB      GET DESCRIPTOR Response CONFIGURATION

Frame 64: 73 bytes on wire (584 bits), 73 bytes captured (584 bits)
    Arrival Time: Sep 21, 2011 14:02:39.125077000 CEST
    Epoch Time: 1316606559.125077000 seconds
    [Time delta from previous captured frame: 0.000321000 seconds]
    [Time delta from previous displayed frame: 0.000321000 seconds]
    [Time since reference or first frame: 364.658109000 seconds]
    Frame Number: 64
    Frame Length: 73 bytes (584 bits)
    Capture Length: 73 bytes (584 bits)
    [Frame is marked: False]
    [Frame is ignored: False]
    [Protocols in frame: usb]
USB URB
    URB id: 0x00000000f37abb00
    URB type: URB_COMPLETE ('C')
    URB transfer type: URB_CONTROL out (0x02)
    Endpoint: 0x80
    Device: 4
    URB bus id: 1
    Device setup request: not relevant ('-')
    Data: present (0)
    URB sec: 1316606559
    URB usec: 125077
    URB status: Success (0)
    URB length [bytes]: 9
    Data length [bytes]: 9
    [Request in: 63]
    [Time from request: 0.000321000 seconds]
    [bInterfaceClass: PRINTER (0x07)]
    CONFIGURATION DESCRIPTOR
        bLength: 9
        bDescriptorType: CONFIGURATION (2)
        wTotalLength: 32
        bNumInterfaces: 1
        bConfigurationValue: 1
        iConfiguration: 0
        Configuration bmAttributes: 0xc0  SELF-POWERED  NO REMOTE-WAKEUP
            1... .... = Must be 1: Must be 1 for USB 1.1 and higher
            .1.. .... = Self-Powered: This device is SELF-POWERED
            ..0. .... = Remote Wakeup: This device does NOT support remote wakeup
        bMaxPower: 1  (2mA)

0000  00 bb 7a f3 00 00 00 00 43 02 80 04 01 00 2d 00   ..z.....C.....-.
0010  5f d2 79 4e 00 00 00 00 95 e8 01 00 00 00 00 00   _.yN............
0020  09 00 00 00 09 00 00 00 00 00 00 00 00 00 00 00   ................
0030  00 00 00 00 00 00 00 00 00 02 00 00 00 00 00 00   ................
0040  09 02 20 00 01 01 00 c0 01                        .. ......

No.     Time        Source                Destination           Protocol Info
     65 364.658149  host                  4.0                   USB      GET DESCRIPTOR Request CONFIGURATION

Frame 65: 64 bytes on wire (512 bits), 64 bytes captured (512 bits)
    Arrival Time: Sep 21, 2011 14:02:39.125117000 CEST
    Epoch Time: 1316606559.125117000 seconds
    [Time delta from previous captured frame: 0.000040000 seconds]
    [Time delta from previous displayed frame: 0.000040000 seconds]
    [Time since reference or first frame: 364.658149000 seconds]
    Frame Number: 65
    Frame Length: 64 bytes (512 bits)
    Capture Length: 64 bytes (512 bits)
    [Frame is marked: False]
    [Frame is ignored: False]
    [Protocols in frame: usb]
USB URB
    URB id: 0x00000000f37abb00
    URB type: URB_SUBMIT ('S')
    URB transfer type: URB_CONTROL out (0x02)
    Endpoint: 0x80
    Device: 4
    URB bus id: 1
    Device setup request: relevant (0)
    Data: not present ('<')
    URB sec: 1316606559
    URB usec: 125117
    URB status: Operation now in progress (-EINPROGRESS) (-115)
    URB length [bytes]: 32
    Data length [bytes]: 0
    [Response in: 66]
    [bInterfaceClass: PRINTER (0x07)]
    URB setup
        bmRequestType: 0x80
            1... .... = Direction: Device-to-host
            .00. .... = Type: Standard (0x00)
            ...0 0000 = Recipient: Device (0x00)
        bRequest: GET DESCRIPTOR (6)
        Descriptor Index: 0x00
        bDescriptorType: CONFIGURATION (2)
        Language Id: no language specified (0x0000)
        wLength: 32

0000  00 bb 7a f3 00 00 00 00 53 02 80 04 01 00 00 3c   ..z.....S......<
0010  5f d2 79 4e 00 00 00 00 bd e8 01 00 8d ff ff ff   _.yN............
0020  20 00 00 00 00 00 00 00 80 06 00 02 00 00 20 00    ............. .
0030  00 00 00 00 00 00 00 00 00 02 00 00 00 00 00 00   ................

No.     Time        Source                Destination           Protocol Info
     66 364.658484  4.0                   host                  USB      GET DESCRIPTOR Response CONFIGURATION

Frame 66: 96 bytes on wire (768 bits), 96 bytes captured (768 bits)
    Arrival Time: Sep 21, 2011 14:02:39.125452000 CEST
    Epoch Time: 1316606559.125452000 seconds
    [Time delta from previous captured frame: 0.000335000 seconds]
    [Time delta from previous displayed frame: 0.000335000 seconds]
    [Time since reference or first frame: 364.658484000 seconds]
    Frame Number: 66
    Frame Length: 96 bytes (768 bits)
    Capture Length: 96 bytes (768 bits)
    [Frame is marked: False]
    [Frame is ignored: False]
    [Protocols in frame: usb]
USB URB
    URB id: 0x00000000f37abb00
    URB type: URB_COMPLETE ('C')
    URB transfer type: URB_CONTROL out (0x02)
    Endpoint: 0x80
    Device: 4
    URB bus id: 1
    Device setup request: not relevant ('-')
    Data: present (0)
    URB sec: 1316606559
    URB usec: 125452
    URB status: Success (0)
    URB length [bytes]: 32
    Data length [bytes]: 32
    [Request in: 65]
    [Time from request: 0.000335000 seconds]
    [bInterfaceClass: PRINTER (0x07)]
    CONFIGURATION DESCRIPTOR
        bLength: 9
        bDescriptorType: CONFIGURATION (2)
        wTotalLength: 32
        bNumInterfaces: 1
        bConfigurationValue: 1
        iConfiguration: 0
        Configuration bmAttributes: 0xc0  SELF-POWERED  NO REMOTE-WAKEUP
            1... .... = Must be 1: Must be 1 for USB 1.1 and higher
            .1.. .... = Self-Powered: This device is SELF-POWERED
            ..0. .... = Remote Wakeup: This device does NOT support remote wakeup
        bMaxPower: 1  (2mA)
    INTERFACE DESCRIPTOR
        bLength: 9
        bDescriptorType: INTERFACE (4)
        bInterfaceNumber: 0
        bAlternateSetting: 0
        bNumEndpoints: 2
        bInterfaceClass: PRINTER (0x07)
        bInterfaceSubClass: 0x01
        bInterfaceProtocol: 0x02
        iInterface: 0
    ENDPOINT DESCRIPTOR
        bLength: 7
        bDescriptorType: ENDPOINT (5)
        bEndpointAddress: 0x01  OUT  Endpoint:1
            0... .... = Direction: OUT Endpoint
            .... 0001 = Endpoint Number: 0x01
        bmAttributes: 0x02
            .... ..10 = Transfertype: Bulk-Transfer (0x02)
            .... 00.. = Synchronisationtype: No Sync (0x00)
            ..00 .... = Behaviourtype: Data-Endpoint (0x00)
        wMaxPacketSize: 512
        bInterval: 0
    ENDPOINT DESCRIPTOR
        bLength: 7
        bDescriptorType: ENDPOINT (5)
        bEndpointAddress: 0x82  IN  Endpoint:2
            1... .... = Direction: IN Endpoint
            .... 0010 = Endpoint Number: 0x02
        bmAttributes: 0x02
            .... ..10 = Transfertype: Bulk-Transfer (0x02)
            .... 00.. = Synchronisationtype: No Sync (0x00)
            ..00 .... = Behaviourtype: Data-Endpoint (0x00)
        wMaxPacketSize: 512
        bInterval: 0

0000  00 bb 7a f3 00 00 00 00 43 02 80 04 01 00 2d 00   ..z.....C.....-.
0010  5f d2 79 4e 00 00 00 00 0c ea 01 00 00 00 00 00   _.yN............
0020  20 00 00 00 20 00 00 00 00 00 00 00 00 00 00 00    ... ...........
0030  00 00 00 00 00 00 00 00 00 02 00 00 00 00 00 00   ................
0040  09 02 20 00 01 01 00 c0 01 09 04 00 00 02 07 01   .. .............
0050  02 00 07 05 01 02 00 02 00 07 05 82 02 00 02 00   ................

No.     Time        Source                Destination           Protocol Info
     67 364.658527  host                  4.0                   USB      GET DESCRIPTOR Request STRING

Frame 67: 64 bytes on wire (512 bits), 64 bytes captured (512 bits)
    Arrival Time: Sep 21, 2011 14:02:39.125495000 CEST
    Epoch Time: 1316606559.125495000 seconds
    [Time delta from previous captured frame: 0.000043000 seconds]
    [Time delta from previous displayed frame: 0.000043000 seconds]
    [Time since reference or first frame: 364.658527000 seconds]
    Frame Number: 67
    Frame Length: 64 bytes (512 bits)
    Capture Length: 64 bytes (512 bits)
    [Frame is marked: False]
    [Frame is ignored: False]
    [Protocols in frame: usb]
USB URB
    URB id: 0x00000000f37abb00
    URB type: URB_SUBMIT ('S')
    URB transfer type: URB_CONTROL out (0x02)
    Endpoint: 0x80
    Device: 4
    URB bus id: 1
    Device setup request: relevant (0)
    Data: not present ('<')
    URB sec: 1316606559
    URB usec: 125495
    URB status: Operation now in progress (-EINPROGRESS) (-115)
    URB length [bytes]: 255
    Data length [bytes]: 0
    [Response in: 68]
    [bInterfaceClass: PRINTER (0x07)]
    URB setup
        bmRequestType: 0x80
            1... .... = Direction: Device-to-host
            .00. .... = Type: Standard (0x00)
            ...0 0000 = Recipient: Device (0x00)
        bRequest: GET DESCRIPTOR (6)
        Descriptor Index: 0x00
        bDescriptorType: STRING (3)
        Language Id: no language specified (0x0000)
        wLength: 255

0000  00 bb 7a f3 00 00 00 00 53 02 80 04 01 00 00 3c   ..z.....S......<
0010  5f d2 79 4e 00 00 00 00 37 ea 01 00 8d ff ff ff   _.yN....7.......
0020  ff 00 00 00 00 00 00 00 80 06 00 03 00 00 ff 00   ................
0030  00 00 00 00 00 00 00 00 00 02 00 00 00 00 00 00   ................

No.     Time        Source                Destination           Protocol Info
     68 364.658859  4.0                   host                  USB      GET DESCRIPTOR Response STRING

Frame 68: 68 bytes on wire (544 bits), 68 bytes captured (544 bits)
    Arrival Time: Sep 21, 2011 14:02:39.125827000 CEST
    Epoch Time: 1316606559.125827000 seconds
    [Time delta from previous captured frame: 0.000332000 seconds]
    [Time delta from previous displayed frame: 0.000332000 seconds]
    [Time since reference or first frame: 364.658859000 seconds]
    Frame Number: 68
    Frame Length: 68 bytes (544 bits)
    Capture Length: 68 bytes (544 bits)
    [Frame is marked: False]
    [Frame is ignored: False]
    [Protocols in frame: usb]
USB URB
    URB id: 0x00000000f37abb00
    URB type: URB_COMPLETE ('C')
    URB transfer type: URB_CONTROL out (0x02)
    Endpoint: 0x80
    Device: 4
    URB bus id: 1
    Device setup request: not relevant ('-')
    Data: present (0)
    URB sec: 1316606559
    URB usec: 125827
    URB status: Success (0)
    URB length [bytes]: 4
    Data length [bytes]: 4
    [Request in: 67]
    [Time from request: 0.000332000 seconds]
    [bInterfaceClass: PRINTER (0x07)]
    STRING DESCRIPTOR
        bLength: 4
        bDescriptorType: STRING (3)
        wLANGID: English (United States) (0x0409)

0000  00 bb 7a f3 00 00 00 00 43 02 80 04 01 00 2d 00   ..z.....C.....-.
0010  5f d2 79 4e 00 00 00 00 83 eb 01 00 00 00 00 00   _.yN............
0020  04 00 00 00 04 00 00 00 00 00 00 00 00 00 00 00   ................
0030  00 00 00 00 00 00 00 00 00 02 00 00 00 00 00 00   ................
0040  04 03 09 04                                       ....

No.     Time        Source                Destination           Protocol Info
     69 364.658878  host                  4.0                   USB      GET DESCRIPTOR Request STRING

Frame 69: 64 bytes on wire (512 bits), 64 bytes captured (512 bits)
    Arrival Time: Sep 21, 2011 14:02:39.125846000 CEST
    Epoch Time: 1316606559.125846000 seconds
    [Time delta from previous captured frame: 0.000019000 seconds]
    [Time delta from previous displayed frame: 0.000019000 seconds]
    [Time since reference or first frame: 364.658878000 seconds]
    Frame Number: 69
    Frame Length: 64 bytes (512 bits)
    Capture Length: 64 bytes (512 bits)
    [Frame is marked: False]
    [Frame is ignored: False]
    [Protocols in frame: usb]
USB URB
    URB id: 0x00000000f37abb00
    URB type: URB_SUBMIT ('S')
    URB transfer type: URB_CONTROL out (0x02)
    Endpoint: 0x80
    Device: 4
    URB bus id: 1
    Device setup request: relevant (0)
    Data: not present ('<')
    URB sec: 1316606559
    URB usec: 125846
    URB status: Operation now in progress (-EINPROGRESS) (-115)
    URB length [bytes]: 255
    Data length [bytes]: 0
    [Response in: 70]
    [bInterfaceClass: PRINTER (0x07)]
    URB setup
        bmRequestType: 0x80
            1... .... = Direction: Device-to-host
            .00. .... = Type: Standard (0x00)
            ...0 0000 = Recipient: Device (0x00)
        bRequest: GET DESCRIPTOR (6)
        Descriptor Index: 0x02
        bDescriptorType: STRING (3)
        Language Id: English (United States) (0x0409)
        wLength: 255

0000  00 bb 7a f3 00 00 00 00 53 02 80 04 01 00 00 3c   ..z.....S......<
0010  5f d2 79 4e 00 00 00 00 96 eb 01 00 8d ff ff ff   _.yN............
0020  ff 00 00 00 00 00 00 00 80 06 02 03 09 04 ff 00   ................
0030  00 00 00 00 00 00 00 00 00 02 00 00 00 00 00 00   ................

No.     Time        Source                Destination           Protocol Info
     70 364.659109  4.0                   host                  USB      GET DESCRIPTOR Response STRING

Frame 70: 86 bytes on wire (688 bits), 86 bytes captured (688 bits)
    Arrival Time: Sep 21, 2011 14:02:39.126077000 CEST
    Epoch Time: 1316606559.126077000 seconds
    [Time delta from previous captured frame: 0.000231000 seconds]
    [Time delta from previous displayed frame: 0.000231000 seconds]
    [Time since reference or first frame: 364.659109000 seconds]
    Frame Number: 70
    Frame Length: 86 bytes (688 bits)
    Capture Length: 86 bytes (688 bits)
    [Frame is marked: False]
    [Frame is ignored: False]
    [Protocols in frame: usb]
USB URB
    URB id: 0x00000000f37abb00
    URB type: URB_COMPLETE ('C')
    URB transfer type: URB_CONTROL out (0x02)
    Endpoint: 0x80
    Device: 4
    URB bus id: 1
    Device setup request: not relevant ('-')
    Data: present (0)
    URB sec: 1316606559
    URB usec: 126077
    URB status: Success (0)
    URB length [bytes]: 22
    Data length [bytes]: 22
    [Request in: 69]
    [Time from request: 0.000231000 seconds]
    [bInterfaceClass: PRINTER (0x07)]
    STRING DESCRIPTOR
        bLength: 22
        bDescriptorType: STRING (3)
        bString: 423 Series

0000  00 bb 7a f3 00 00 00 00 43 02 80 04 01 00 2d 00   ..z.....C.....-.
0010  5f d2 79 4e 00 00 00 00 7d ec 01 00 00 00 00 00   _.yN....}.......
0020  16 00 00 00 16 00 00 00 00 00 00 00 00 00 00 00   ................
0030  00 00 00 00 00 00 00 00 00 02 00 00 00 00 00 00   ................
0040  16 03 34 00 32 00 33 00 20 00 53 00 65 00 72 00   ..4.2.3. .S.e.r.
0050  69 00 65 00 73 00                                 i.e.s.

No.     Time        Source                Destination           Protocol Info
     71 364.659138  host                  4.0                   USB      GET DESCRIPTOR Request STRING

Frame 71: 64 bytes on wire (512 bits), 64 bytes captured (512 bits)
    Arrival Time: Sep 21, 2011 14:02:39.126106000 CEST
    Epoch Time: 1316606559.126106000 seconds
    [Time delta from previous captured frame: 0.000029000 seconds]
    [Time delta from previous displayed frame: 0.000029000 seconds]
    [Time since reference or first frame: 364.659138000 seconds]
    Frame Number: 71
    Frame Length: 64 bytes (512 bits)
    Capture Length: 64 bytes (512 bits)
    [Frame is marked: False]
    [Frame is ignored: False]
    [Protocols in frame: usb]
USB URB
    URB id: 0x00000000f37abb00
    URB type: URB_SUBMIT ('S')
    URB transfer type: URB_CONTROL out (0x02)
    Endpoint: 0x80
    Device: 4
    URB bus id: 1
    Device setup request: relevant (0)
    Data: not present ('<')
    URB sec: 1316606559
    URB usec: 126106
    URB status: Operation now in progress (-EINPROGRESS) (-115)
    URB length [bytes]: 255
    Data length [bytes]: 0
    [Response in: 72]
    [bInterfaceClass: PRINTER (0x07)]
    URB setup
        bmRequestType: 0x80
            1... .... = Direction: Device-to-host
            .00. .... = Type: Standard (0x00)
            ...0 0000 = Recipient: Device (0x00)
        bRequest: GET DESCRIPTOR (6)
        Descriptor Index: 0x01
        bDescriptorType: STRING (3)
        Language Id: English (United States) (0x0409)
        wLength: 255

0000  00 bb 7a f3 00 00 00 00 53 02 80 04 01 00 00 3c   ..z.....S......<
0010  5f d2 79 4e 00 00 00 00 9a ec 01 00 8d ff ff ff   _.yN............
0020  ff 00 00 00 00 00 00 00 80 06 01 03 09 04 ff 00   ................
0030  00 00 00 00 00 00 00 00 00 02 00 00 00 00 00 00   ................

No.     Time        Source                Destination           Protocol Info
     72 364.659482  4.0                   host                  USB      GET DESCRIPTOR Response STRING

Frame 72: 94 bytes on wire (752 bits), 94 bytes captured (752 bits)
    Arrival Time: Sep 21, 2011 14:02:39.126450000 CEST
    Epoch Time: 1316606559.126450000 seconds
    [Time delta from previous captured frame: 0.000344000 seconds]
    [Time delta from previous displayed frame: 0.000344000 seconds]
    [Time since reference or first frame: 364.659482000 seconds]
    Frame Number: 72
    Frame Length: 94 bytes (752 bits)
    Capture Length: 94 bytes (752 bits)
    [Frame is marked: False]
    [Frame is ignored: False]
    [Protocols in frame: usb]
USB URB
    URB id: 0x00000000f37abb00
    URB type: URB_COMPLETE ('C')
    URB transfer type: URB_CONTROL out (0x02)
    Endpoint: 0x80
    Device: 4
    URB bus id: 1
    Device setup request: not relevant ('-')
    Data: present (0)
    URB sec: 1316606559
    URB usec: 126450
    URB status: Success (0)
    URB length [bytes]: 30
    Data length [bytes]: 30
    [Request in: 71]
    [Time from request: 0.000344000 seconds]
    [bInterfaceClass: PRINTER (0x07)]
    STRING DESCRIPTOR
        bLength: 30
        bDescriptorType: STRING (3)
        bString: KONICA MINOLTA

0000  00 bb 7a f3 00 00 00 00 43 02 80 04 01 00 2d 00   ..z.....C.....-.
0010  5f d2 79 4e 00 00 00 00 f2 ed 01 00 00 00 00 00   _.yN............
0020  1e 00 00 00 1e 00 00 00 00 00 00 00 00 00 00 00   ................
0030  00 00 00 00 00 00 00 00 00 02 00 00 00 00 00 00   ................
0040  1e 03 4b 00 4f 00 4e 00 49 00 43 00 41 00 20 00   ..K.O.N.I.C.A. .
0050  4d 00 49 00 4e 00 4f 00 4c 00 54 00 41 00         M.I.N.O.L.T.A.

No.     Time        Source                Destination           Protocol Info
     73 364.659722  host                  4.0                   USB      SET CONFIGURATION Request

Frame 73: 64 bytes on wire (512 bits), 64 bytes captured (512 bits)
    Arrival Time: Sep 21, 2011 14:02:39.126690000 CEST
    Epoch Time: 1316606559.126690000 seconds
    [Time delta from previous captured frame: 0.000240000 seconds]
    [Time delta from previous displayed frame: 0.000240000 seconds]
    [Time since reference or first frame: 364.659722000 seconds]
    Frame Number: 73
    Frame Length: 64 bytes (512 bits)
    Capture Length: 64 bytes (512 bits)
    [Frame is marked: False]
    [Frame is ignored: False]
    [Protocols in frame: usb]
USB URB
    URB id: 0x00000000f37abb00
    URB type: URB_SUBMIT ('S')
    URB transfer type: URB_CONTROL out (0x02)
    Endpoint: 0x00
    Device: 4
    URB bus id: 1
    Device setup request: relevant (0)
    Data: present (0)
    URB sec: 1316606559
    URB usec: 126690
    URB status: Operation now in progress (-EINPROGRESS) (-115)
    URB length [bytes]: 0
    Data length [bytes]: 0
    [Response in: 74]
    [bInterfaceClass: PRINTER (0x07)]
    URB setup
        bmRequestType: 0x00
            0... .... = Direction: Host-to-device
            .00. .... = Type: Standard (0x00)
            ...0 0000 = Recipient: Device (0x00)
        bRequest: SET CONFIGURATION (9)
        bConfigurationValue: 1
        wIndex: 0
        wLength: 0

0000  00 bb 7a f3 00 00 00 00 53 02 00 04 01 00 00 00   ..z.....S.......
0010  5f d2 79 4e 00 00 00 00 e2 ee 01 00 8d ff ff ff   _.yN............
0020  00 00 00 00 00 00 00 00 00 09 01 00 00 00 00 00   ................
0030  00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00   ................

No.     Time        Source                Destination           Protocol Info
     74 364.659850  4.0                   host                  USB      SET CONFIGURATION Response

Frame 74: 64 bytes on wire (512 bits), 64 bytes captured (512 bits)
    Arrival Time: Sep 21, 2011 14:02:39.126818000 CEST
    Epoch Time: 1316606559.126818000 seconds
    [Time delta from previous captured frame: 0.000128000 seconds]
    [Time delta from previous displayed frame: 0.000128000 seconds]
    [Time since reference or first frame: 364.659850000 seconds]
    Frame Number: 74
    Frame Length: 64 bytes (512 bits)
    Capture Length: 64 bytes (512 bits)
    [Frame is marked: False]
    [Frame is ignored: False]
    [Protocols in frame: usb]
USB URB
    URB id: 0x00000000f37abb00
    URB type: URB_COMPLETE ('C')
    URB transfer type: URB_CONTROL out (0x02)
    Endpoint: 0x00
    Device: 4
    URB bus id: 1
    Device setup request: not relevant ('-')
    Data: not present ('>')
    URB sec: 1316606559
    URB usec: 126818
    URB status: Success (0)
    URB length [bytes]: 0
    Data length [bytes]: 0
    [Request in: 73]
    [Time from request: 0.000128000 seconds]
    [bInterfaceClass: PRINTER (0x07)]

0000  00 bb 7a f3 00 00 00 00 43 02 00 04 01 00 2d 3e   ..z.....C.....->
0010  5f d2 79 4e 00 00 00 00 62 ef 01 00 00 00 00 00   _.yN....b.......
0020  00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00   ................
0030  00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00   ................

No.     Time        Source                Destination           Protocol Info
     75 364.660619  host                  4.0                   USB      SET INTERFACE Request

Frame 75: 64 bytes on wire (512 bits), 64 bytes captured (512 bits)
    Arrival Time: Sep 21, 2011 14:02:39.127587000 CEST
    Epoch Time: 1316606559.127587000 seconds
    [Time delta from previous captured frame: 0.000769000 seconds]
    [Time delta from previous displayed frame: 0.000769000 seconds]
    [Time since reference or first frame: 364.660619000 seconds]
    Frame Number: 75
    Frame Length: 64 bytes (512 bits)
    Capture Length: 64 bytes (512 bits)
    [Frame is marked: False]
    [Frame is ignored: False]
    [Protocols in frame: usb]
USB URB
    URB id: 0x00000000f37abb00
    URB type: URB_SUBMIT ('S')
    URB transfer type: URB_CONTROL out (0x02)
    Endpoint: 0x00
    Device: 4
    URB bus id: 1
    Device setup request: relevant (0)
    Data: present (0)
    URB sec: 1316606559
    URB usec: 127587
    URB status: Operation now in progress (-EINPROGRESS) (-115)
    URB length [bytes]: 0
    Data length [bytes]: 0
    [Response in: 76]
    [bInterfaceClass: PRINTER (0x07)]
    URB setup
        bmRequestType: 0x01
            0... .... = Direction: Host-to-device
            .00. .... = Type: Standard (0x00)
            ...0 0001 = Recipient: Interface (0x01)
        bRequest: SET INTERFACE (11)
        bAlternateSetting: 0
        wInterface: 0
        wLength: 0

0000  00 bb 7a f3 00 00 00 00 53 02 00 04 01 00 00 00   ..z.....S.......
0010  5f d2 79 4e 00 00 00 00 63 f2 01 00 8d ff ff ff   _.yN....c.......
0020  00 00 00 00 00 00 00 00 01 0b 00 00 00 00 00 00   ................
0030  00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00   ................

No.     Time        Source                Destination           Protocol Info
     76 364.661233  4.0                   host                  USB      SET INTERFACE Response

Frame 76: 64 bytes on wire (512 bits), 64 bytes captured (512 bits)
    Arrival Time: Sep 21, 2011 14:02:39.128201000 CEST
    Epoch Time: 1316606559.128201000 seconds
    [Time delta from previous captured frame: 0.000614000 seconds]
    [Time delta from previous displayed frame: 0.000614000 seconds]
    [Time since reference or first frame: 364.661233000 seconds]
    Frame Number: 76
    Frame Length: 64 bytes (512 bits)
    Capture Length: 64 bytes (512 bits)
    [Frame is marked: False]
    [Frame is ignored: False]
    [Protocols in frame: usb]
USB URB
    URB id: 0x00000000f37abb00
    URB type: URB_COMPLETE ('C')
    URB transfer type: URB_CONTROL out (0x02)
    Endpoint: 0x00
    Device: 4
    URB bus id: 1
    Device setup request: not relevant ('-')
    Data: not present ('>')
    URB sec: 1316606559
    URB usec: 128201
    URB status: Success (0)
    URB length [bytes]: 0
    Data length [bytes]: 0
    [Request in: 75]
    [Time from request: 0.000614000 seconds]
    [bInterfaceClass: PRINTER (0x07)]

0000  00 bb 7a f3 00 00 00 00 43 02 00 04 01 00 2d 3e   ..z.....C.....->
0010  5f d2 79 4e 00 00 00 00 c9 f4 01 00 00 00 00 00   _.yN............
0020  00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00   ................
0030  00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00   ................

No.     Time        Source                Destination           Protocol Info
     77 364.661350  host                  4.0                   USB      URB_CONTROL out

Frame 77: 64 bytes on wire (512 bits), 64 bytes captured (512 bits)
    Arrival Time: Sep 21, 2011 14:02:39.128318000 CEST
    Epoch Time: 1316606559.128318000 seconds
    [Time delta from previous captured frame: 0.000117000 seconds]
    [Time delta from previous displayed frame: 0.000117000 seconds]
    [Time since reference or first frame: 364.661350000 seconds]
    Frame Number: 77
    Frame Length: 64 bytes (512 bits)
    Capture Length: 64 bytes (512 bits)
    [Frame is marked: False]
    [Frame is ignored: False]
    [Protocols in frame: usb]
USB URB
    URB id: 0x00000000f37abb00
    URB type: URB_SUBMIT ('S')
    URB transfer type: URB_CONTROL out (0x02)
    Endpoint: 0x80
    Device: 4
    URB bus id: 1
    Device setup request: relevant (0)
    Data: not present ('<')
    URB sec: 1316606559
    URB usec: 128318
    URB status: Operation now in progress (-EINPROGRESS) (-115)
    URB length [bytes]: 1023
    Data length [bytes]: 0
    [Response in: 78]
    [bInterfaceClass: PRINTER (0x07)]
    URB setup
        bmRequestType: 0xa1
            1... .... = Direction: Device-to-host
            .01. .... = Type: Class (0x01)
            ...0 0001 = Recipient: Interface (0x01)
        bRequest: 0
        wValue: 0x0000
        wIndex: 0
        wLength: 1023

0000  00 bb 7a f3 00 00 00 00 53 02 80 04 01 00 00 3c   ..z.....S......<
0010  5f d2 79 4e 00 00 00 00 3e f5 01 00 8d ff ff ff   _.yN....>.......
0020  ff 03 00 00 00 00 00 00 a1 00 00 00 00 00 ff 03   ................
0030  00 00 00 00 00 00 00 00 00 02 00 00 00 00 00 00   ................

No.     Time        Source                Destination           Protocol Info
     78 364.662110  4.0                   host                  USB      URB_CONTROL out

Frame 78: 197 bytes on wire (1576 bits), 197 bytes captured (1576 bits)
    Arrival Time: Sep 21, 2011 14:02:39.129078000 CEST
    Epoch Time: 1316606559.129078000 seconds
    [Time delta from previous captured frame: 0.000760000 seconds]
    [Time delta from previous displayed frame: 0.000760000 seconds]
    [Time since reference or first frame: 364.662110000 seconds]
    Frame Number: 78
    Frame Length: 197 bytes (1576 bits)
    Capture Length: 197 bytes (1576 bits)
    [Frame is marked: False]
    [Frame is ignored: False]
    [Protocols in frame: usb]
USB URB
    URB id: 0x00000000f37abb00
    URB type: URB_COMPLETE ('C')
    URB transfer type: URB_CONTROL out (0x02)
    Endpoint: 0x80
    Device: 4
    URB bus id: 1
    Device setup request: not relevant ('-')
    Data: present (0)
    URB sec: 1316606559
    URB usec: 129078
    URB status: Success (0)
    URB length [bytes]: 133
    Data length [bytes]: 133
    [Request in: 77]
    [Time from request: 0.000760000 seconds]
    [bInterfaceClass: PRINTER (0x07)]
    CONTROL response data

0000  00 bb 7a f3 00 00 00 00 43 02 80 04 01 00 2d 00   ..z.....C.....-.
0010  5f d2 79 4e 00 00 00 00 36 f8 01 00 00 00 00 00   _.yN....6.......
0020  85 00 00 00 85 00 00 00 00 00 00 00 00 00 00 00   ................
0030  00 00 00 00 00 00 00 00 00 02 00 00 00 00 00 00   ................
0040  00 85 4d 46 47 3a 4b 4f 4e 49 43 41 20 4d 49 4e   ..MFG:KONICA MIN
0050  4f 4c 54 41 3b 43 4d 44 3a 50 53 2c 50 4f 53 54   OLTA;CMD:PS,POST
0060  53 43 52 49 50 54 2c 50 43 4c 3b 4d 44 4c 3a 34   SCRIPT,PCL;MDL:4
0070  32 33 20 53 65 72 69 65 73 3b 43 4c 41 53 53 3a   23 Series;CLASS:
0080  50 52 49 4e 54 45 52 3b 43 4f 4d 4d 45 4e 54 3a   PRINTER;COMMENT:
0090  4b 4f 4e 49 43 41 5f 4d 49 4e 4f 4c 54 41 5f 62   KONICA_MINOLTA_b
00a0  69 7a 68 75 62 5f 34 32 33 20 53 65 72 69 65 73   izhub_423 Series
00b0  3b 41 43 54 49 56 45 20 43 4f 4d 4d 41 4e 44 20   ;ACTIVE COMMAND 
00c0  53 45 54 3a 3b                                    SET:;

No.     Time        Source                Destination           Protocol Info
     79 368.057974  host                  4.2                   USB      URB_BULK out

Frame 79: 64 bytes on wire (512 bits), 64 bytes captured (512 bits)
    Arrival Time: Sep 21, 2011 14:02:42.524942000 CEST
    Epoch Time: 1316606562.524942000 seconds
    [Time delta from previous captured frame: 3.395864000 seconds]
    [Time delta from previous displayed frame: 3.395864000 seconds]
    [Time since reference or first frame: 368.057974000 seconds]
    Frame Number: 79
    Frame Length: 64 bytes (512 bits)
    Capture Length: 64 bytes (512 bits)
    [Frame is marked: False]
    [Frame is ignored: False]
    [Protocols in frame: usb]
USB URB
    URB id: 0x00000000f0c9df80
    URB type: URB_SUBMIT ('S')
    URB transfer type: URB_BULK out (0x03)
    Endpoint: 0x82
    Device: 4
    URB bus id: 1
    Device setup request: not relevant ('-')
    Data: not present ('<')
    URB sec: 1316606562
    URB usec: 524942
    URB status: Operation now in progress (-EINPROGRESS) (-115)
    URB length [bytes]: 1024
    Data length [bytes]: 0
    [Response in: 82]
    [bInterfaceClass: PRINTER (0x07)]

0000  80 df c9 f0 00 00 00 00 53 03 82 04 01 00 2d 3c   ........S.....-<
0010  62 d2 79 4e 00 00 00 00 8e 02 08 00 8d ff ff ff   b.yN............
0020  00 04 00 00 00 00 00 00 00 00 00 00 00 00 00 00   ................
0030  00 00 00 00 00 00 00 00 00 02 00 00 00 00 00 00   ................

No.     Time        Source                Destination           Protocol Info
     80 368.058000  host                  4.0                   USB      URB_CONTROL out

Frame 80: 64 bytes on wire (512 bits), 64 bytes captured (512 bits)
    Arrival Time: Sep 21, 2011 14:02:42.524968000 CEST
    Epoch Time: 1316606562.524968000 seconds
    [Time delta from previous captured frame: 0.000026000 seconds]
    [Time delta from previous displayed frame: 0.000026000 seconds]
    [Time since reference or first frame: 368.058000000 seconds]
    Frame Number: 80
    Frame Length: 64 bytes (512 bits)
    Capture Length: 64 bytes (512 bits)
    [Frame is marked: False]
    [Frame is ignored: False]
    [Protocols in frame: usb]
USB URB
    URB id: 0x00000000f0c9dd00
    URB type: URB_SUBMIT ('S')
    URB transfer type: URB_CONTROL out (0x02)
    Endpoint: 0x80
    Device: 4
    URB bus id: 1
    Device setup request: relevant (0)
    Data: not present ('<')
    URB sec: 1316606562
    URB usec: 524968
    URB status: Operation now in progress (-EINPROGRESS) (-115)
    URB length [bytes]: 1023
    Data length [bytes]: 0
    [Response in: 81]
    [bInterfaceClass: PRINTER (0x07)]
    URB setup
        bmRequestType: 0xa1
            1... .... = Direction: Device-to-host
            .01. .... = Type: Class (0x01)
            ...0 0001 = Recipient: Interface (0x01)
        bRequest: 0
        wValue: 0x0000
        wIndex: 0
        wLength: 1023

0000  00 dd c9 f0 00 00 00 00 53 02 80 04 01 00 00 3c   ........S......<
0010  62 d2 79 4e 00 00 00 00 a8 02 08 00 8d ff ff ff   b.yN............
0020  ff 03 00 00 00 00 00 00 a1 00 00 00 00 00 ff 03   ................
0030  00 00 00 00 00 00 00 00 00 02 00 00 00 00 00 00   ................

No.     Time        Source                Destination           Protocol Info
     81 368.058213  4.0                   host                  USB      URB_CONTROL out

Frame 81: 197 bytes on wire (1576 bits), 197 bytes captured (1576 bits)
    Arrival Time: Sep 21, 2011 14:02:42.525181000 CEST
    Epoch Time: 1316606562.525181000 seconds
    [Time delta from previous captured frame: 0.000213000 seconds]
    [Time delta from previous displayed frame: 0.000213000 seconds]
    [Time since reference or first frame: 368.058213000 seconds]
    Frame Number: 81
    Frame Length: 197 bytes (1576 bits)
    Capture Length: 197 bytes (1576 bits)
    [Frame is marked: False]
    [Frame is ignored: False]
    [Protocols in frame: usb]
USB URB
    URB id: 0x00000000f0c9dd00
    URB type: URB_COMPLETE ('C')
    URB transfer type: URB_CONTROL out (0x02)
    Endpoint: 0x80
    Device: 4
    URB bus id: 1
    Device setup request: not relevant ('-')
    Data: present (0)
    URB sec: 1316606562
    URB usec: 525181
    URB status: Success (0)
    URB length [bytes]: 133
    Data length [bytes]: 133
    [Request in: 80]
    [Time from request: 0.000213000 seconds]
    [bInterfaceClass: PRINTER (0x07)]
    CONTROL response data

0000  00 dd c9 f0 00 00 00 00 43 02 80 04 01 00 2d 00   ........C.....-.
0010  62 d2 79 4e 00 00 00 00 7d 03 08 00 00 00 00 00   b.yN....}.......
0020  85 00 00 00 85 00 00 00 00 00 00 00 00 00 00 00   ................
0030  00 00 00 00 00 00 00 00 00 02 00 00 00 00 00 00   ................
0040  00 85 4d 46 47 3a 4b 4f 4e 49 43 41 20 4d 49 4e   ..MFG:KONICA MIN
0050  4f 4c 54 41 3b 43 4d 44 3a 50 53 2c 50 4f 53 54   OLTA;CMD:PS,POST
0060  53 43 52 49 50 54 2c 50 43 4c 3b 4d 44 4c 3a 34   SCRIPT,PCL;MDL:4
0070  32 33 20 53 65 72 69 65 73 3b 43 4c 41 53 53 3a   23 Series;CLASS:
0080  50 52 49 4e 54 45 52 3b 43 4f 4d 4d 45 4e 54 3a   PRINTER;COMMENT:
0090  4b 4f 4e 49 43 41 5f 4d 49 4e 4f 4c 54 41 5f 62   KONICA_MINOLTA_b
00a0  69 7a 68 75 62 5f 34 32 33 20 53 65 72 69 65 73   izhub_423 Series
00b0  3b 41 43 54 49 56 45 20 43 4f 4d 4d 41 4e 44 20   ;ACTIVE COMMAND 
00c0  53 45 54 3a 3b                                    SET:;

No.     Time        Source                Destination           Protocol Info
     82 368.058579  4.2                   host                  USB      URB_BULK out

Frame 82: 64 bytes on wire (512 bits), 64 bytes captured (512 bits)
    Arrival Time: Sep 21, 2011 14:02:42.525547000 CEST
    Epoch Time: 1316606562.525547000 seconds
    [Time delta from previous captured frame: 0.000366000 seconds]
    [Time delta from previous displayed frame: 0.000366000 seconds]
    [Time since reference or first frame: 368.058579000 seconds]
    Frame Number: 82
    Frame Length: 64 bytes (512 bits)
    Capture Length: 64 bytes (512 bits)
    [Frame is marked: False]
    [Frame is ignored: False]
    [Protocols in frame: usb]
USB URB
    URB id: 0x00000000f0c9df80
    URB type: URB_COMPLETE ('C')
    URB transfer type: URB_BULK out (0x03)
    Endpoint: 0x82
    Device: 4
    URB bus id: 1
    Device setup request: not relevant ('-')
    Data: present (0)
    URB sec: 1316606562
    URB usec: 525547
    URB status: No such file or directory (-ENOENT) (-2)
    URB length [bytes]: 0
    Data length [bytes]: 0
    [Request in: 79]
    [Time from request: 0.000605000 seconds]
    [bInterfaceClass: PRINTER (0x07)]

0000  80 df c9 f0 00 00 00 00 43 03 82 04 01 00 2d 00   ........C.....-.
0010  62 d2 79 4e 00 00 00 00 eb 04 08 00 fe ff ff ff   b.yN............
0020  00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00   ................
0030  00 00 00 00 00 00 00 00 00 02 00 00 00 00 00 00   ................
