<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="8.2.1">
<drawing>
<board>
<plain>
<wire x1="1.27" y1="40.64" x2="23.8" y2="40.64" width="0" layer="20"/>
<wire x1="23.8" y1="40.64" x2="23.8" y2="83.81" width="0" layer="20"/>
<wire x1="23.8" y1="83.81" x2="1.27" y2="83.81" width="0" layer="20"/>
<wire x1="1.27" y1="83.81" x2="1.27" y2="40.64" width="0" layer="20"/>
<text>I²C</text>
<text>1-wire</text>
<text>V0.1</text>
<text>NodeMCU I²C and 1-wire breakout board</text>
<text>Licensed under CERN OHL v.1.2</text>
<text>Designed by 
R. Kainhofer, 2017</text>
<text>D0</text>
</plain>
<libraries>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Connectors&lt;/h3&gt;
This library contains electrically-functional connectors. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X15">
<description>&lt;h3&gt;Plated Through Hole -15 Pin&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:15&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_15&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X06">
<description>&lt;h3&gt;Plated Through Hole - 6 Pin&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:6&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_06&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X05">
<description>&lt;h3&gt;Plated Through Hole - 5 Pin&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:5&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_05&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="J1" library="SparkFun-Connectors" package="1X15" value="NodeMCU">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J2" library="SparkFun-Connectors" package="1X15" value="Breakout">
<attribute name="NAME"/>
</element>
<element name="J10" library="SparkFun-Connectors" package="1X05" value="G">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J11" library="SparkFun-Connectors" package="1X05" value="V">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J3" library="SparkFun-Connectors" package="1X06" value="V">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CONN-08437"/>
<attribute name="VALUE"/>
</element>
<element name="J4" library="SparkFun-Connectors" package="1X06" value="G">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CONN-08437"/>
<attribute name="VALUE"/>
</element>
<element name="J5" library="SparkFun-Connectors" package="1X06" value="SCL">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CONN-08437"/>
<attribute name="VALUE"/>
</element>
<element name="J6" library="SparkFun-Connectors" package="1X06" value="SDA">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CONN-08437"/>
<attribute name="VALUE"/>
</element>
<element name="J7" library="SparkFun-Connectors" package="1X06" value="G">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CONN-08437"/>
<attribute name="VALUE"/>
</element>
<element name="J8" library="SparkFun-Connectors" package="1X06" value="D">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CONN-08437"/>
<attribute name="VALUE"/>
</element>
<element name="J9" library="SparkFun-Connectors" package="1X06" value="V">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CONN-08437"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="D3">
<contactref element="J2" pad="12"/>
<contactref element="J1" pad="12"/>
</signal>
<signal name="D4">
<contactref element="J2" pad="11"/>
<contactref element="J1" pad="11"/>
</signal>
<signal name="D8">
<contactref element="J2" pad="5"/>
<contactref element="J1" pad="5"/>
</signal>
<signal name="TX">
<contactref element="J2" pad="3"/>
<contactref element="J1" pad="3"/>
</signal>
<signal name="RX">
<contactref element="J2" pad="4"/>
<contactref element="J1" pad="4"/>
</signal>
<signal name="D5">
<contactref element="J2" pad="8"/>
<contactref element="J1" pad="8"/>
<contactref element="J8" pad="6"/>
<contactref element="J8" pad="5"/>
<contactref element="J8" pad="4"/>
<contactref element="J8" pad="3"/>
<contactref element="J8" pad="2"/>
<contactref element="J8" pad="1"/>
</signal>
<signal name="3V3">
<contactref element="J2" pad="10"/>
<contactref element="J1" pad="10"/>
<contactref element="J3" pad="6"/>
<contactref element="J3" pad="5"/>
<contactref element="J3" pad="4"/>
<contactref element="J3" pad="3"/>
<contactref element="J3" pad="2"/>
<contactref element="J3" pad="1"/>
</signal>
<signal name="3V3_2">
<contactref element="J2" pad="1"/>
<contactref element="J1" pad="1"/>
<contactref element="J11" pad="1"/>
<contactref element="J11" pad="2"/>
<contactref element="J11" pad="3"/>
<contactref element="J11" pad="4"/>
<contactref element="J11" pad="5"/>
<contactref element="J9" pad="6"/>
<contactref element="J9" pad="5"/>
<contactref element="J9" pad="4"/>
<contactref element="J9" pad="3"/>
<contactref element="J9" pad="2"/>
<contactref element="J9" pad="1"/>
</signal>
<signal name="D7">
<contactref element="J2" pad="6"/>
<contactref element="J1" pad="6"/>
</signal>
<signal name="N$6">
<contactref element="J2" pad="15"/>
<contactref element="J1" pad="15"/>
</signal>
<signal name="D1_SCL">
<contactref element="J2" pad="14"/>
<contactref element="J1" pad="14"/>
<contactref element="J5" pad="1"/>
<contactref element="J5" pad="2"/>
<contactref element="J5" pad="3"/>
<contactref element="J5" pad="4"/>
<contactref element="J5" pad="5"/>
<contactref element="J5" pad="6"/>
</signal>
<signal name="D6">
<contactref element="J2" pad="7"/>
<contactref element="J1" pad="7"/>
</signal>
<signal name="GND">
<contactref element="J4" pad="6"/>
<contactref element="J4" pad="5"/>
<contactref element="J4" pad="4"/>
<contactref element="J4" pad="3"/>
<contactref element="J4" pad="2"/>
<contactref element="J4" pad="1"/>
<contactref element="J2" pad="9"/>
<contactref element="J1" pad="9"/>
<contactref element="J7" pad="6"/>
<contactref element="J7" pad="5"/>
<contactref element="J7" pad="4"/>
<contactref element="J7" pad="3"/>
<contactref element="J7" pad="2"/>
<contactref element="J7" pad="1"/>
</signal>
<signal name="D2_SDA">
<contactref element="J6" pad="6"/>
<contactref element="J6" pad="5"/>
<contactref element="J6" pad="4"/>
<contactref element="J6" pad="3"/>
<contactref element="J6" pad="2"/>
<contactref element="J6" pad="1"/>
<contactref element="J2" pad="13"/>
<contactref element="J1" pad="13"/>
</signal>
<signal name="GND_2">
<contactref element="J2" pad="2"/>
<contactref element="J1" pad="2"/>
<contactref element="J10" pad="5"/>
<contactref element="J10" pad="4"/>
<contactref element="J10" pad="3"/>
<contactref element="J10" pad="2"/>
<contactref element="J10" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
